#*******************************************************************
#
# $Source: /sc/CvsTree/sc/gen/src/form/ased_acqu.form,v $
#
# Copyright (c) 1995 - 2008
# BRUKER BioSpin GmbH
# D-76287 Rheinstetten, Germany
#
# All Rights Reserved
#
#
# $Id: ased_acqu.form,v 1.37 2019/02/13 07:59:38 chjo Exp $
#*******************************************************************
EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"====== General ======"
NAME		PULPROG
END
NAME		TD
END
NAME		SW
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"sweep width"
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP,FnMODE)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP,FnMODE)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
                TEXT	"acquisition time"
END
NAME		RG
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3f usec"
		TEXT	"dwell time "
END
NAME		DE
		FORMAT	"%14.2f usec"
END
T_NAME		GRPDLY
		TYPE	R64
		SUBRANGE 0 1e38
		CLASS	ACQU
		REL	"GRPDLY=GRPDLY"
		INV_REL	"GRPDLY=GRPDLY"				
		UNIT	"no"
		TEXT	"group delay of digital filter"
		FORMAT	"%14.0f"
		NONEDIT
END
T_NAME		cnst4
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst4=plw4"
		INV_REL	"D[0]=cnst4"
		UNIT	"no"
		TEXT	"cnst4=plw4"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst12
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst12=plw12"
		INV_REL	"D[0]=cnst12"
		UNIT	"no"
		TEXT	"cnst12=plw12"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst22
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst22=plw22"
		INV_REL	"D[0]=cnst22"
		UNIT	"no"
		TEXT	"cnst22=plw22"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst23
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst23=plw23"
		INV_REL	"D[0]=cnst23"
		UNIT	"no"
		TEXT	"cnst23=plw23"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst24
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst24=plw24"
		INV_REL	"D[0]=cnst24"
		UNIT	"no"
		TEXT	"cnst24=plw24"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst25
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst25=plw25"
		INV_REL	"D[0]=cnst25"
		UNIT	"no"
		TEXT	"cnst25=plw25"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst26
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst26=plw26"
		INV_REL	"D[0]=cnst26"
		UNIT	"no"
		TEXT	"cnst26=plw26"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst27
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst27=plw27"
		INV_REL	"D[0]=cnst27"
		UNIT	"no"
		TEXT	"cnst27=plw27"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst28
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst28=spw25"
		INV_REL	"D[0]=cnst28"
		UNIT	"no"
		TEXT	"cnst28=spw25"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst29
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst29=spw30"
		INV_REL	"D[0]=cnst29"
		UNIT	"no"
		TEXT	"cnst29=spw30"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst31
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst31=plw31"
		INV_REL	"D[0]=cnst31"
		UNIT	"no"
		TEXT	"cnst31=plw31"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		cnst41
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"cnst41=plw41"
		INV_REL	"D[0]=cnst41"
		UNIT	"no"
		TEXT	"cnst41=plw41"
		FORMAT	"%14.6f"
		NONEDIT
END
T_NAME		d0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d0=0.2u"
		INV_REL	"D[0]=d0"
		UNIT	"sec"
		TEXT	"d0=0.2u"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		D1
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D1=D[1]"
INV_REL	"D[1]=D1"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"relaxation delay"
END
T_NAME		d10
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d10=0.2u"
		INV_REL	"D[0]=d10"
		UNIT	"sec"
		TEXT	"d10=0.2u"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		d11
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d11=30m"
		INV_REL	"D[0]=d11"
		UNIT	"sec"
		TEXT		"delay for disk i/o, 30ms"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		D14
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D14=D[14]"
INV_REL	"D[14]=D14"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"bigT1, 650 us"
END
T_NAME		D16
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D16=D[16]"
INV_REL	"D[16]=D16"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"gradient recovery delay, 200us"
END
T_NAME		D20
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D20=D[20]"
INV_REL	"D[20]=D20"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"taua, H to C, 1.8ms"
END
T_NAME		D21
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D21=D[21]"
INV_REL	"D[21]=D21"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"taub, refocus JHC for 13C mag"
END
T_NAME		D22
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D22=D[22]"
INV_REL	"D[22]=D22"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"tauc, Ca to CO transfer, 3.6 ms "
END
T_NAME		D23
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D23=D[23]"
INV_REL	"D[23]=D23"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"taud, Ca-CO J refocus, 4.9 ms "
END
T_NAME		D24
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D24=D[24]"
INV_REL	"D[24]=D24"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"taue, N-CO J evolve, 12.4 ms"
END
T_NAME		D25
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D25=D[25]"
INV_REL	"D[25]=D25"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"bigTN, t2 evolv, N-CO refocus, 12.4 ms"
END
T_NAME		D26
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D26=D[26]"
INV_REL	"D[26]=D26"
UNIT	"sec"
FORMAT	"%14.9f sec"
		TEXT		"tauf, 1/4JNH, ~ 2.4 ms"
END
NAME		DS
		TEXT	"number of dummy scans"
END
T_NAME		in0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"in0=inf1/2"
		INV_REL	"D[0]=in0"
		UNIT	"sec"
		TEXT	"in0=inf1/2"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		in10
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"in10=inf2/2"
		INV_REL	"D[0]=in10"
		UNIT	"sec"
		TEXT	"in10=inf2/2"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		INF1
TYPE	R64
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"INF1=INF[1]"
INV_REL	"INF[1]=INF1"
UNIT	"usec"
FORMAT	"%14.4f usec"
TEXT	"increment for F1"
NONEDIT
END
T_NAME		INF2
TYPE	R64
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"INF2=INF[2]"
INV_REL	"INF[2]=INF2"
UNIT	"usec"
FORMAT	"%14.4f usec"
TEXT	"increment for F2"
NONEDIT
END
T_NAME		L7
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"L7=L[7]"
INV_REL	"L[7]=L7"
FORMAT	"%14.0f"
		TEXT		"ncyc, number of times flopsy is repeated; total_time = pwcdip*94.22*ncyc"
END
NAME		NS
		TEXT	"scans to execute"
END
T_NAME		P41
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P41=P[41]"
INV_REL	"P[41]=P41"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"2H decoupling"
END
NAME		TDav	
		TEXT	"number of averages in nD"
END
NAME		ZGOPTNS
		TEXT 	"options for zg"
END
T_NAME		bigT1
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"bigT1 = d14"
		INV_REL	"D[0]=bigT1"
		UNIT	"sec"
		TEXT	"bigT1 = d14"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		bigTN
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"bigTN = d25"
		INV_REL	"D[0]=bigTN"
		UNIT	"sec"
		TEXT	"bigTN = d25"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		ncyc
		TYPE	I32
		SUBRANGE 0 2147483647
		CLASS	ACQU
		REL	"ncyc = l7"
		INV_REL	"D[0]=ncyc"
		UNIT	"no"
		TEXT	"ncyc = l7"
		FORMAT	"%14d"
		NONEDIT
END
T_NAME		ni
		TYPE	I32
		SUBRANGE 0 2147483647
		CLASS	ACQU
		REL	" ni = td1/2"
		INV_REL	"D[0]=ni"
		UNIT	"no"
		TEXT	" ni = td1/2"
		FORMAT	"%14d"
		NONEDIT
END
T_NAME		pwcdip
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwcdip=p22"
		INV_REL	"D[0]=pwcdip"
		UNIT	"usec"
		TEXT	"pwcdip=p22"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwddec
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwddec=p41"
		INV_REL	"D[0]=pwddec"
		UNIT	"usec"
		TEXT	"pwddec=p41"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		taua
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"taua = d20"
		INV_REL	"D[0]=taua"
		UNIT	"sec"
		TEXT	"taua = d20"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		taub
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"taub = d21"
		INV_REL	"D[0]=taub"
		UNIT	"sec"
		TEXT	"taub = d21"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		tauc
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"tauc = d22"
		INV_REL	"D[0]=tauc"
		UNIT	"sec"
		TEXT	"tauc = d22"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		taud
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"taud = d23"
		INV_REL	"D[0]=taud"
		UNIT	"sec"
		TEXT	"taud = d23"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		taue
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"taue = d24"
		INV_REL	"D[0]=taue"
		UNIT	"sec"
		TEXT	"taue = d24"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		tauf
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"tauf = d26"
		INV_REL	"D[0]=tauf"
		UNIT	"sec"
		TEXT	"tauf = d26"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		zeta1
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"zeta1=0.1u"
		INV_REL	"D[0]=zeta1"
		UNIT	"sec"
		TEXT	"zeta1=0.1u"
		FORMAT	"%14.10f sec"
		NONEDIT
END
T_NAME		zetacount
		TYPE	I32
		SUBRANGE 0 2147483647
		CLASS	ACQU
		REL	"zetacount=1"
		INV_REL	"D[0]=zetacount"
		UNIT	"no"
		TEXT	"zetacount=1"
		FORMAT	"%14d"
		NONEDIT
END
HEADER		"======== CHANNEL f1 ========"
NAME		SFO1
FORMAT	"%14.7f MHz"
TEXT	"frequency of ch. 1"
END
NAME		O1
FORMAT	"%14.2f Hz"
TEXT	"frequency of ch. 1"
END
T_NAME		O1P
TYPE	R64
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"O1P=O1/BF1"
INV_REL	"O1=O1P*BF1"
UNIT	"ppm"
FORMAT	"%14.3f ppm"
TEXT	"frequency of ch. 1"
END
NAME		NUC1
NONEDIT
TEXT	"nucleus for channel 1"
END
NAME		CPDPRG[1]
TEXT	"file name for cpd1"
END
T_NAME		P1
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P1=P[1]"
INV_REL	"P[1]=P1"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwh"
END
T_NAME		P12
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P12=P[12]"
INV_REL	"P[12]=P12"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwmlev - 1H 90 for waltz16dec at power pl12"
END
T_NAME		PCPD1
TYPE	R32
CLASS	ACQU
SUBRANGE 0 1e38
REL	"PCPD1=PCPD[1]"
INV_REL	"PCPD[1]=PCPD1"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	"cpd pulse for ch. 1"
END
T_NAME		PLW1
TYPE	R32
CLASS	ACQU
SUBRANGE 0 82.9245
REL	"PLW1=PLW[1]"
INV_REL	"PLW[1]=PLW1"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"tpwr - power level for pwh"
END
T_NAME		PLdB1
TYPE	R32
CLASS	ACQU
SUBRANGE -19.2868 1000
REL	"if(PLW[1]>0)PLdB1=-10*log(PLW[1])/LN10;else PLdB1=1000;"
INV_REL	"PLW[1]=0;if(PLdB1<1000)PLW[1]=pow(10.0,(-PLdB1)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL1 in dB"
END
T_NAME		PLW12
TYPE	R32
CLASS	ACQU
SUBRANGE 0 82.9245
REL	"PLW12=PLW[12]"
INV_REL	"PLW[12]=PLW12"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"tpwrml - power level for 1H waltz16"
END
T_NAME		PLdB12
TYPE	R32
CLASS	ACQU
SUBRANGE -19.2868 1000
REL	"if(PLW[12]>0)PLdB12=-10*log(PLW[12])/LN10;else PLdB12=1000;"
INV_REL	"PLW[12]=0;if(PLdB12<1000)PLW[12]=pow(10.0,(-PLdB12)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL12 in dB"
END
T_NAME		pwh
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwh=p1"
		INV_REL	"D[0]=pwh"
		UNIT	"usec"
		TEXT	"pwh=p1"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwmlev
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwmlev=p12"
		INV_REL	"D[0]=pwmlev"
		UNIT	"usec"
		TEXT	"pwmlev=p12"
		FORMAT	"%14.2f usec"
		NONEDIT
END
HEADER		"======== CHANNEL f2 ========"
NAME		SFO2
FORMAT	"%14.7f MHz"
TEXT	"frequency of ch. 2"
END
NAME		O2
FORMAT	"%14.2f Hz"
TEXT	"frequency of ch. 2"
END
T_NAME		O2P
TYPE	R64
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"O2P=O2/BF2"
INV_REL	"O2=O2P*BF2"
UNIT	"ppm"
FORMAT	"%14.3f ppm"
TEXT	"frequency of ch. 2"
END
NAME		NUC2
NONEDIT
TEXT	"nucleus for channel 2"
END
T_NAME		CNST2
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST2=CNST[2]"
INV_REL	"CNST[2]=CNST2"
FORMAT	"%14.7f"
		TEXT		"(58-43)ppm offset in Hz"
END
T_NAME		CNST3
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST3=CNST[3]"
INV_REL	"CNST[3]=CNST3"
FORMAT	"%14.7f"
		TEXT		"(176-43)ppm offset in Hz"
END
NAME		CPDPRG[2]
		TEXT		"flopsy transfer"
END
NAME		CPDPRG[5]
		TEXT		"CO decoupling while sit at 43 ppm"
END
NAME		CPDPRG[6]
		TEXT		"Ca decoupling while carbon carrier at 176 ppm (mag is 15N)"
END
NAME		CPDPRG[7]
		TEXT		"Cb decoupling while sit at 58 ppm"
END
T_NAME		P2
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P2=P[2]"
INV_REL	"P[2]=P2"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwc"
END
T_NAME		P22
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P22=P[22]"
INV_REL	"P[22]=P22"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwcdip - 13C 90 at pl22 for C tocsy about 30 ms"
END
T_NAME		P23
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P23=P[23]"
INV_REL	"P[23]=P23"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwCOdec - pattern length us @ spw23 "
END
T_NAME		P24
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P24=P[24]"
INV_REL	"P[24]=P24"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwCO90c, pwca90b"
END
T_NAME		P25
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P25=P[25]"
INV_REL	"P[25]=P25"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwCO180b,pwCa180b,pwCO180c,pwCa180c"
END
T_NAME		P26
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P26=P[26]"
INV_REL	"P[26]=P26"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwCadec - pattern length us @ spw26"
END
T_NAME		P27
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P27=P[27]"
INV_REL	"P[27]=P27"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwCbdec - pattern length us @ spw27"
END
T_NAME		PLW2
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW2=PLW[2]"
INV_REL	"PLW[2]=PLW2"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dhpwr - power level for C 90 and 180"
END
T_NAME		PLdB2
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[2]>0)PLdB2=-10*log(PLW[2])/LN10;else PLdB2=1000;"
INV_REL	"PLW[2]=0;if(PLdB2<1000)PLW[2]=pow(10.0,(-PLdB2)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL2 in dB"
END
T_NAME		PLW21
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW21=PLW[21]"
INV_REL	"PLW[21]=PLW21"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dpwr - low power level for C (dec)"
END
T_NAME		PLdB21
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[21]>0)PLdB21=-10*log(PLW[21])/LN10;else PLdB21=1000;"
INV_REL	"PLW[21]=0;if(PLdB21<1000)PLW[21]=pow(10.0,(-PLdB21)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL21 in dB"
END
T_NAME		PLW22
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW22=PLW[22]"
INV_REL	"PLW[22]=PLW22"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dpwrdip - power level for C tocsy"
END
T_NAME		PLdB22
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[22]>0)PLdB22=-10*log(PLW[22])/LN10;else PLdB22=1000;"
INV_REL	"PLW[22]=0;if(PLdB22<1000)PLW[22]=pow(10.0,(-PLdB22)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL22 in dB"
END
T_NAME		PLW23
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW23=PLW[23]"
INV_REL	"PLW[23]=PLW23"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dpwrcodec - power level for CO seduce decoupling"
END
T_NAME		PLdB23
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[23]>0)PLdB23=-10*log(PLW[23])/LN10;else PLdB23=1000;"
INV_REL	"PLW[23]=0;if(PLdB23<1000)PLW[23]=pow(10.0,(-PLdB23)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL23 in dB"
END
T_NAME		PLW24
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW24=PLW[24]"
INV_REL	"PLW[24]=PLW24"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dhpwrb - power level for Ca90b/CO90b"
END
T_NAME		PLdB24
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[24]>0)PLdB24=-10*log(PLW[24])/LN10;else PLdB24=1000;"
INV_REL	"PLW[24]=0;if(PLdB24<1000)PLW[24]=pow(10.0,(-PLdB24)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL24 in dB"
END
T_NAME		PLW25
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW25=PLW[25]"
INV_REL	"PLW[25]=PLW25"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dvhpwrb - power level for CO180b/Ca180b"
END
T_NAME		PLdB25
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[25]>0)PLdB25=-10*log(PLW[25])/LN10;else PLdB25=1000;"
INV_REL	"PLW[25]=0;if(PLdB25<1000)PLW[25]=pow(10.0,(-PLdB25)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL25 in dB"
END
T_NAME		PLW26
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW26=PLW[26]"
INV_REL	"PLW[26]=PLW26"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dpwrcadec - power level for Ca seduce decoupling"
END
T_NAME		PLdB26
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[26]>0)PLdB26=-10*log(PLW[26])/LN10;else PLdB26=1000;"
INV_REL	"PLW[26]=0;if(PLdB26<1000)PLW[26]=pow(10.0,(-PLdB26)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL26 in dB"
END
T_NAME		PLW27
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"PLW27=PLW[27]"
INV_REL	"PLW[27]=PLW27"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dpwrcbdec - power level for sel Cb decoupling"
END
T_NAME		PLdB27
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(PLW[27]>0)PLdB27=-10*log(PLW[27])/LN10;else PLdB27=1000;"
INV_REL	"PLW[27]=0;if(PLdB27<1000)PLW[27]=pow(10.0,(-PLdB27)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL27 in dB"
END
NAME		SPNAM[23]
		TEXT		"File name for CO decoupling sitting at 43 ppm"
END
T_NAME		SPOAL23
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL23=SPOAL[23]"
INV_REL	"SPOAL[23]=SPOAL23"
FORMAT	"%14.3f"
TEXT	"phase alignment of freq. offset in SP23"
END
T_NAME		SPOFFS23
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS23=SPOFFS[23]"
INV_REL	"SPOFFS[23]=SPOFFS23"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	"offset frequency for SP23"
END
NAME		SPNAM[25]
		TEXT		"File name for D/sq(3), +118p"
END
T_NAME		SPOAL25
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL25=SPOAL[25]"
INV_REL	"SPOAL[25]=SPOAL25"
FORMAT	"%14.3f"
TEXT	"phase alignment of freq. offset in SP25"
END
T_NAME		SPOFFS25
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS25=SPOFFS[25]"
INV_REL	"SPOFFS[25]=SPOFFS25"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	"offset frequency for SP25"
END
T_NAME		SPW25
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"SPW25=SPW[25]"
INV_REL	"SPW[25]=SPW25"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"power level for pwco180b (shaped pulse) when carrier is on Ca"
END
T_NAME		SPdB25
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(SPW[25]>0)SPdB25=-10*log(SPW[25])/LN10;elseSPdB25=1000;"
INV_REL	"SPW[25]=0;if(SPdB25<1000)SPW[25]=pow(10.0,(-SPdB25)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f -dBW"
TEXT	"power SPW25 in -dBW"
END
NAME		SPNAM[26]
		TEXT		"File name for Ca decoupling during 15N t2"
END
T_NAME		SPOAL26
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL26=SPOAL[26]"
INV_REL	"SPOAL[26]=SPOAL26"
FORMAT	"%14.3f"
TEXT	"phase alignment of freq. offset in SP26"
END
T_NAME		SPOFFS26
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS26=SPOFFS[26]"
INV_REL	"SPOFFS[26]=SPOFFS26"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	"offset frequency for SP26"
END
NAME		SPNAM[27]
		TEXT		"File name for Cb decoupling during Ca to Co transfer"
END
T_NAME		SPOAL27
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL27=SPOAL[27]"
INV_REL	"SPOAL[27]=SPOAL27"
FORMAT	"%14.3f"
TEXT	"phase alignment of freq. offset in SP27"
END
T_NAME		SPOFFS27
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS27=SPOFFS[27]"
INV_REL	"SPOFFS[27]=SPOFFS27"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	"offset frequency for SP27"
END
NAME		SPNAM[30]
		TEXT		"File name for Ca D/sq(3), -118p"
END
T_NAME		SPOAL30
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL30=SPOAL[30]"
INV_REL	"SPOAL[30]=SPOAL30"
FORMAT	"%14.3f"
TEXT	"phase alignment of freq. offset in SP30"
END
T_NAME		SPOFFS30
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS30=SPOFFS[30]"
INV_REL	"SPOFFS[30]=SPOFFS30"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	"offset frequency for SP30"
END
T_NAME		SPW30
TYPE	R32
CLASS	ACQU
SUBRANGE 0 418.037
REL	"SPW30=SPW[30]"
INV_REL	"SPW[30]=SPW30"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"power level for pwca180c (shaped pulse) when carrier is on CO"
END
T_NAME		SPdB30
TYPE	R32
CLASS	ACQU
SUBRANGE -26.3122 1000
REL	"if(SPW[30]>0)SPdB30=-10*log(SPW[30])/LN10;elseSPdB30=1000;"
INV_REL	"SPW[30]=0;if(SPdB30<1000)SPW[30]=pow(10.0,(-SPdB30)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f -dBW"
TEXT	"power SPW30 in -dBW"
END
T_NAME		pwc
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwc=p2"
		INV_REL	"D[0]=pwc"
		UNIT	"usec"
		TEXT	"pwc=p2"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwca180b
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwca180b=p25"
		INV_REL	"D[0]=pwca180b"
		UNIT	"usec"
		TEXT	"pwca180b=p25"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwca180c
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwca180c=p25"
		INV_REL	"D[0]=pwca180c"
		UNIT	"usec"
		TEXT	"pwca180c=p25"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwca90b
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwca90b=p24"
		INV_REL	"D[0]=pwca90b"
		UNIT	"usec"
		TEXT	"pwca90b=p24"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwco180b
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwco180b=p25"
		INV_REL	"D[0]=pwco180b"
		UNIT	"usec"
		TEXT	"pwco180b=p25"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwco180c
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwco180c=p25"
		INV_REL	"D[0]=pwco180c"
		UNIT	"usec"
		TEXT	"pwco180c=p25"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		pwco90c
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwco90c=p24"
		INV_REL	"D[0]=pwco90c"
		UNIT	"usec"
		TEXT	"pwco90c=p24"
		FORMAT	"%14.2f usec"
		NONEDIT
END
HEADER		"======== CHANNEL f3 ========"
NAME		SFO3
FORMAT	"%14.7f MHz"
TEXT	"frequency of ch. 3"
END
NAME		O3
FORMAT	"%14.2f Hz"
TEXT	"frequency of ch. 3"
END
T_NAME		O3P
TYPE	R64
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"O3P=O3/BF3"
INV_REL	"O3=O3P*BF3"
UNIT	"ppm"
FORMAT	"%14.3f ppm"
TEXT	"frequency of ch. 3"
END
NAME		NUC3
NONEDIT
TEXT	"nucleus for channel 3"
END
NAME		CPDPRG[3]
TEXT	"file name for cpd3"
END
T_NAME		P3
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P3=P[3]"
INV_REL	"P[3]=P3"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"pwn"
END
T_NAME		PCPD3
TYPE	R32
CLASS	ACQU
SUBRANGE 0 1e38
REL	"PCPD3=PCPD[3]"
INV_REL	"PCPD[3]=PCPD3"
UNIT	"usec"
FORMAT	"%14.2f usec"
		TEXT		"1/dmf2 - 90 degree pulse for cpd3"
END
T_NAME		PLW3
TYPE	R32
CLASS	ACQU
SUBRANGE 0 485.271
REL	"PLW3=PLW[3]"
INV_REL	"PLW[3]=PLW3"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dhpwr2 - power level for pwn"
END
T_NAME		PLdB3
TYPE	R32
CLASS	ACQU
SUBRANGE -26.9598 1000
REL	"if(PLW[3]>0)PLdB3=-10*log(PLW[3])/LN10;else PLdB3=1000;"
INV_REL	"PLW[3]=0;if(PLdB3<1000)PLW[3]=pow(10.0,(-PLdB3)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL3 in dB"
END
T_NAME		PLW31
TYPE	R32
CLASS	ACQU
SUBRANGE 0 485.271
REL	"PLW31=PLW[31]"
INV_REL	"PLW[31]=PLW31"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"dpwr2 - power level for 15N cpd"
END
T_NAME		PLdB31
TYPE	R32
CLASS	ACQU
SUBRANGE -26.9598 1000
REL	"if(PLW[31]>0)PLdB31=-10*log(PLW[31])/LN10;else PLdB31=1000;"
INV_REL	"PLW[31]=0;if(PLdB31<1000)PLW[31]=pow(10.0,(-PLdB31)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL31 in dB"
END
T_NAME		pwn
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwn=p3"
		INV_REL	"D[0]=pwn"
		UNIT	"usec"
		TEXT	"pwn=p3"
		FORMAT	"%14.2f usec"
		NONEDIT
END
HEADER		"======== CHANNEL f4 ========"
NAME		SFO4
FORMAT	"%14.7f MHz"
TEXT	"frequency of ch. 4"
END
NAME		O4
FORMAT	"%14.2f Hz"
TEXT	"frequency of ch. 4"
END
T_NAME		O4P
TYPE	R64
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"O4P=O4/BF4"
INV_REL	"O4=O4P*BF4"
UNIT	"ppm"
FORMAT	"%14.3f ppm"
TEXT	"frequency of ch. 4"
END
NAME		NUC4
NONEDIT
TEXT	"nucleus for channel 4"
END
NAME		CPDPRG[4]
TEXT	"file name for cpd4"
END
T_NAME		P4
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P4=P[4]"
INV_REL	"P[4]=P4"
UNIT	"usec"
FORMAT	"%14.3f usec"
		TEXT		"2H high power pulse, 90"
END
T_NAME		PCPD4
TYPE	R32
CLASS	ACQU
SUBRANGE 0 1e38
REL	"PCPD4=PCPD[4]"
INV_REL	"PCPD[4]=PCPD4"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	"cpd pulse for ch. 4"
END
T_NAME		PLW4
TYPE	R32
CLASS	ACQU
SUBRANGE 0 111.325
REL	"PLW4=PLW[4]"
INV_REL	"PLW[4]=PLW4"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"power level for 2H pulses"
END
T_NAME		PLdB4
TYPE	R32
CLASS	ACQU
SUBRANGE -20.5659 1000
REL	"if(PLW[4]>0)PLdB4=-10*log(PLW[4])/LN10;else PLdB4=1000;"
INV_REL	"PLW[4]=0;if(PLdB4<1000)PLW[4]=pow(10.0,(-PLdB4)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL4 in dB"
END
T_NAME		PLW41
TYPE	R32
CLASS	ACQU
SUBRANGE 0 111.325
REL	"PLW41=PLW[41]"
INV_REL	"PLW[41]=PLW41"
UNIT	"W"
FORMAT	"%14.5g W"
		TEXT		"power level for 2H decoupling"
END
T_NAME		PLdB41
TYPE	R32
CLASS	ACQU
SUBRANGE -20.5659 1000
REL	"if(PLW[41]>0)PLdB41=-10*log(PLW[41])/LN10;else PLdB41=1000;"
INV_REL	"PLW[41]=0;if(PLdB41<1000)PLW[41]=pow(10.0,(-PLdB41)/10.0)"
UNIT	"dB"
FORMAT	"%14.2f dB"
TEXT	"power PL41 in dB"
END
T_NAME		pwd
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"pwd=p4"
		INV_REL	"D[0]=pwd"
		UNIT	"usec"
		TEXT	"pwd=p4"
		FORMAT	"%14.2f usec"
		NONEDIT
END
HEADER		"====== GRADIENT CHANNEL ====="
NAME		GPNAM[0]
TEXT	"file name for gp0 "
END
T_NAME		GPZ0
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ0=GPZ[0]"
INV_REL	"GPZ[0]=GPZ0"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 0"
END
NAME		GPNAM[1]
TEXT	"file name for gp1 "
END
T_NAME		GPZ1
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ1=GPZ[1]"
INV_REL	"GPZ[1]=GPZ1"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 1"
END
NAME		GPNAM[2]
TEXT	"file name for gp2 "
END
T_NAME		GPZ2
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ2=GPZ[2]"
INV_REL	"GPZ[2]=GPZ2"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 2"
END
NAME		GPNAM[3]
TEXT	"file name for gp3 "
END
T_NAME		GPZ3
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ3=GPZ[3]"
INV_REL	"GPZ[3]=GPZ3"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 3"
END
NAME		GPNAM[4]
TEXT	"file name for gp4 "
END
T_NAME		GPZ4
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ4=GPZ[4]"
INV_REL	"GPZ[4]=GPZ4"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 4"
END
NAME		GPNAM[5]
TEXT	"file name for gp5 "
END
T_NAME		GPZ5
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ5=GPZ[5]"
INV_REL	"GPZ[5]=GPZ5"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 5"
END
NAME		GPNAM[6]
TEXT	"file name for gp6 "
END
T_NAME		GPZ6
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ6=GPZ[6]"
INV_REL	"GPZ[6]=GPZ6"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 6"
END
NAME		GPNAM[7]
TEXT	"file name for gp7 "
END
T_NAME		GPZ7
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ7=GPZ[7]"
INV_REL	"GPZ[7]=GPZ7"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 7"
END
NAME		GPNAM[8]
TEXT	"file name for gp8 "
END
T_NAME		GPZ8
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ8=GPZ[8]"
INV_REL	"GPZ[8]=GPZ8"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 8"
END
NAME		GPNAM[9]
TEXT	"file name for gp9 "
END
T_NAME		GPZ9
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ9=GPZ[9]"
INV_REL	"GPZ[9]=GPZ9"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	"z-gradient strength 9"
END
T_NAME		P50
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P50=P[50]"
INV_REL	"P[50]=P50"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 50"
END
T_NAME		P51
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P51=P[51]"
INV_REL	"P[51]=P51"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 51"
END
T_NAME		P52
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P52=P[52]"
INV_REL	"P[52]=P52"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 52"
END
T_NAME		P53
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P53=P[53]"
INV_REL	"P[53]=P53"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 53"
END
T_NAME		P54
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P54=P[54]"
INV_REL	"P[54]=P54"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 54"
END
T_NAME		P55
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P55=P[55]"
INV_REL	"P[55]=P55"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 55"
END
T_NAME		P56
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P56=P[56]"
INV_REL	"P[56]=P56"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 56"
END
T_NAME		P57
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P57=P[57]"
INV_REL	"P[57]=P57"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 57"
END
T_NAME		P58
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P58=P[58]"
INV_REL	"P[58]=P58"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 58"
END
T_NAME		P59
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P59=P[59]"
INV_REL	"P[59]=P59"
UNIT	"usec"
FORMAT	"%14.3f usec"
TEXT	"pulse 59"
END
