CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.1/conf/instr/spect/uxnmr.info
Date         : Mon Apr  8 13:37:59 2013
Release      : TopSpin Acquisition Version 3.1-pl6
Installed in : /opt/topspin3.1
Host         : magneto9001
OS           : CentOS release 5.6 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : nmrsu (NMR Administrator (nmrsu))
Description  : Avance III 900
Location     : University of Minnesota
System       : Avance III NMR spectrometer
1H-frequency : 900.21 MHz
Order Number : 10027829
Configured in: /opt/topspin3.1/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/02418 ECL 06.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 130219
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AV  R  5.0 REC-1  AQS RXAD1000 Z102118/301 ECL 05.00
     3   0x34 0xc9   0x1        X  1.3 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x29   0x8    AD  S  3.6 SGU-1  AQS SGU/2 1000 Z103082/00863 ECL 03.06 FPGA-Vs=AF
     5   0x25 0x29   0x8    AD  S  3.6 SGU-2  AQS SGU/2 1000 Z103082/00864 ECL 03.06 FPGA-Vs=AF
     6   0x26 0x29   0x8    AD  S  3.6 SGU-3  AQS SGU/2 1000 Z103082/00865 ECL 03.06 FPGA-Vs=AF
     7   0x27 0x29   0x8    AD  S  3.6 SGU-4  AQS SGU/2 1000 Z103082/00866 ECL 03.06 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345095_0328 W1345095/0328 ECL 20:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR: W1345095/0328 ECL 20
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1635 ECL 2
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5802 ECL 50
BLA_W1345097_0152 W1345097/0152 ECL 1:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0152 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0967 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5070 ECL 50
LTRX Z109895/00005 ECL 00.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 900: Z109895/00005 ECL 00.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20111004
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 900: Z109895/00005 ECL 00.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00476 ECL 02.03
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00471 ECL 01.03

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.254:/dev/tty04

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.254:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.9%/0.5deg, reflection meter)
                 PN=Z103209, SN=00010 from 20110411
    Module  2 : XBB31P 2HS
                 PN=Z003510, SN=00043 from 20110218
    Module  3 : 13C
                 PN=Z003528, SN=00029 from 20110324
    Module  4 : 15N
                 PN=Z003534, SN=00031 from 20091110
    Module  5 : 2H
                 PN=Z003477, SN=00043 from 20110325


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAX1000 E 6-405MHZ INR W1345095/0328 at TCP/IP 149.236.99.252)
SGU1 AUX  output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249)
SGU2 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX1000 E 6-405MHZ INR W1345095/0328 at TCP/IP 149.236.99.252)
SGU4 NORM output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249)
SGU4 AUX  output -> input 3 of transmitter 1 (BLAX1000 E 6-405MHZ INR W1345095/0328 at TCP/IP 149.236.99.252)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX1000 E 6-405MHZ INR W1345095/0328 at TCP/IP 149.236.99.252) amplifier X-1000W uses blanking 1
transmitter 1 (BLAX1000 E 6-405MHZ INR W1345095/0328 at TCP/IP 149.236.99.252) amplifier X-300W uses blanking 1
transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249) amplifier 1H-100W uses blanking 2
transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249) amplifier X-500W uses blanking 3
transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0152 at TCP/IP 149.236.99.249) amplifier 2H-250W needs no blanking
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 900 Z109895/00005 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

