CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.3/conf/instr/spect/uxnmr.info
Date         : Thu Jun 10 11:49:03 2021
Release      : TopSpin 3.6.3
Installed in : /opt/topspin3.6.3
Host         : mbdrx800
OS           : CentOS Linux release 7.8.2003 (Core)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1729 MHz)
User         : kroon (Gerard Kroon)
System       : Avance III 800 NMR spectrometer
1H-frequency : 800.13 MHz
Description  : Avance III
Configured in: mbdrx800:/opt/topspin3.6.3/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU1: AQS DRU-E Z102520/02181 ECL 06.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AW  R  4.5 REC-1  AQS RXAD1000 Z102118/270 ECL 04.05
     3   0x34 0xc9   0x1        X  1.2 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x29   0x8    AD  S  3.5 SGU-1  AQS SGU/2 1000 Z103082/00740 ECL 03.05 FPGA-Vs=AE  (needs update to version AF)
     5   0x25 0x29   0x8    AE  S  3.5 SGU-2  AQS SGU/2 1000 Z103082/00741 ECL 03.05 FPGA-Vs=AF
     6   0x26 0x29   0x8    AE  S  3.5 SGU-3  AQS SGU/2 1000 Z103082/00742 ECL 03.05 FPGA-Vs=AF
     7   0x27 0x29   0x8    AE  S  3.5 SGU-4  AQS SGU/2 1000 Z103082/00743 ECL 03.05 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0362 W1345093/0362 ECL 1:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0362 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1338 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5231 ECL 50
BLA_W1345093_0354 W1345093/0354 ECL 1:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0354 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1325 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5176 ECL 50
BLA_W1345097_0164 W1345097/0164 ECL 1:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0164 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1035 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5258 ECL 50
LTRX Z109893/00016 ECL 01.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00016 ECL 01.00

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0112
- TCP/IP address   = 149.236.99.94
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20191111
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00016 ECL 01.00
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00185 ECL 02.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00163 ECL 01.01

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty05

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.90:/dev/tty01

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003465, SN=00084 from 20050822
    Module  2 : XBB31P 2HS
                PN=Z003509, SN=00102 from 20050822
    Module  3 : 2H
                PN=Z003476, SN=00084 from 20050920
    Module  4 : 13C
                PN=Z003527, SN=00070 from 20050718
    Module  5 : 15N
                PN=Z003533, SN=00068 from 20051025



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected via DPP to GREAT 3-10 Gradient Amplifier Unit W1213762/0112

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 800 W1345097/0164 at TCP/IP 149.236.99.91)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0354 at TCP/IP 149.236.99.92)
SGU2 NORM output -> input 2 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 800 W1345097/0164 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0354 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0362 at TCP/IP 149.236.99.93)
SGU4 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0362 at TCP/IP 149.236.99.93)
SGU4 AUX  output -> input 4 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 800 W1345097/0164 at TCP/IP 149.236.99.91)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0362 at TCP/IP 149.236.99.93:
- amplifier X-500W uses blanking 4

transmitter 2 = BLAX500 E 6-365MHZ INR W1345093/0354 at TCP/IP 149.236.99.92:
- amplifier X-500W uses blanking 3

transmitter 3 = BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 800 W1345097/0164 at TCP/IP 149.236.99.91:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 800 Z109893/00016 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


