CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Mon Jul  6 18:11:00 2020
Release      : TopSpin 4.0.9
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.0.143.20200525
CPU          : Intel(R) Core(TM) i7-4700EQ CPU @ 2.40GHz (8 cores at 2284 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 800 NMR spectrometer
1H-frequency : 800.25 MHz
Description  : CAB AV4 800 MHZ EXT
Location     : rm 1047 Chemistry Bldg.  Ann Arbor, MI
Bruker Order : 10246612
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- EPU: AV4 EPU Embedded Processing Unit H153448/00115 ECL 01.00
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00416 ECL 01.04
  Location: slot 1 in rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20190906082218
  Devices: MTD at /dev/mtd1, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00415 ECL 01.04
  Location: slot 2 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20190906082218
  Devices: MTD at /dev/mtd4, DRX at /dev/bbu/drx4.5, RTD at /dev/bbu/rtd4.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00414 ECL 01.04
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.22 via PCIe #5
  Firmware Version: 20190906082218
  Devices: MTD at /dev/mtd7, DRX at /dev/bbu/drx5.5, RTD at /dev/bbu/rtd5.4
  Sequencer: FCube
  - FCube3
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00413 ECL 01.04
  Location: slot 4 in rack 1
  Connection: at IP 192.168.180.26 via PCIe #6
  Firmware Version: 20190906082218
  Devices: MTD at /dev/mtd10, DRX at /dev/bbu/drx6.5, RTD at /dev/bbu/rtd6.4
  Sequencer: FCube
  - FCube4
- GTU: AV4 GT-CONTROLLER UNIT Z148393/00112 ECL 01.00
  Location: slot 6 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20190906085855
  Devices: MTD at /dev/mtd13, RTD at /dev/bbu/rtd9.4, GPROC at /dev/bbu/gproc9.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00417 ECL 01.04
  Location: slot 7 in rack 1
  Connection: at IP 192.168.180.42 via PCIe #10
  Firmware Version: 20190906082218
  Devices: MTD at /dev/mtd16, DRX at /dev/bbu/drx10.5, RTD at /dev/bbu/rtd10.4
  Sequencer: FCube
  - FCube5
- PSM-A: AV4 PSM-A Z149510/00146 ECL 01.03
- HPPR/2 COVER2: HPPR/2 Cover2 Z124567/02257 ECL 00.03
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.8%/0.3deg, reflection meter without CRP-Bias capability)
                  PN=Z103208, SN=00277 from 20170202
      Module  2 : 2H
                  PN=Z003476, SN=00366 from 20170510
      Module  3 : 13C
                  PN=Z003527, SN=00358 from 20170216
      Module  4 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111096, SN=00221 from 20170123
      Module  5 : 15N
                  PN=Z003533, SN=00360 from 20170413
      Module  6 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111096, SN=00225 from 20170512
      Module  7 : 31P
                  PN=Z102452, SN=00210 from 20160810
  
- HPLNA 19F1H: HPLNA 1H MODULE 800 Z103208/00277 ECL 02.04
- 2H: HPPR/2 2H MODULE 800 Z003476/00366 ECL 07.00
- 13C: HPPR/2 13C MODULE 800 Z003527/00358 ECL 07.00
- HPLNA BB31P: HPLNA XBB 31P MODULE 800 Z111096/00221 ECL 04.02
- 15N: HPPR/2 15N MODULE 800 Z003533/00360 ECL 07.00
- HPLNA BB31P: HPLNA XBB 31P MODULE 800 Z111096/00225 ECL 04.03
- 31P: HPPR/2 31P MODULE 800 Z102452/00210 ECL 07.00
- RACK: AV4 AQS CHASSIS Z149500/00161 ECL 00.02
- PSM-48V: AV4 PSM-48V Z149850/00262 ECL 01.01
- PSM-D: AV4 PSM-D Z149520/00137 ECL 00.02
- FANTRAY: AV4 AQS FAN TRAY Z149501/0152 ECL 00.01
- REF 1200: AV4 REFERENCE 1200 Z148270/00143 ECL 01.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W149107-000014 W149107/000014 ECL 10:
- TCP/IP address = 192.168.99.15
- Firmware VS    = 20181126
- Amplifier      = BLA2H 200-900: W149107/000014 ECL 10
- Controller     = BLA CONTROL BOARD 7: W133936/000684 ECL 20
BLA-W144056-000012 W144056/000012 ECL 00:
- TCP/IP address = 192.168.99.14
- Firmware VS    = 20181126
- Amplifier      = AV4 BLAH500 700-900: W144056/000012 ECL 00
- Controller     = BLA CONTROL BOARD 7: W133936/000581 ECL 20
BLA-W144059-000058 W144059/000058 ECL 00:
- TCP/IP address = 192.168.99.13
- Firmware VS    = 20181126
- Amplifier      = AV4 BLABB500 15-600: W144059/000058 ECL 00
- Controller     = BLA CONTROL BOARD 7: W133936/001106 ECL 20
BLA-W152248-000019 W152248/000019 ECL 00:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20181126
- Amplifier      = AV4 BLA2BB500 15-600: W152248/000019 ECL 00
- Controller     = BLA CONTROL BOARD 7: W133936/000571 ECL 20
LTRX Z109893/00256 ECL 02.01:
- TCP/IP address = 192.168.99.11
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00256 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11
- ELCB firmware version = 20190521
- ELCB = BSMS/2 ELCB: Z100818/06802 ECL 07.02
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- Shim System = BOSS3-SB
- SCB channels = 40
- Shim matrix file: 292722ea.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 Z7 Z8 XZ5 YZ5 (X2-Y2)Z3 (X2-Y2)Z4 (X2-Y2)Z5 XYZ3 XYZ4 XYZ5
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00256 ECL 02.01
- Lock: on L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03898 ECL 05.02
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/00142 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11

Cryo Cooling Control Unit: RETROFIT-CU - AV4 RETROFIT RS232 CU JAC Z161936/00030
- TCP/IP address   = 192.168.98.2

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99
Line Distribution Unit 2: PDU2
- TCP/IP address   = 192.168.99.101


Gradient Controller cable connections
--------------------------------------------------------------------


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 2 (AV4 BLAH500 700-900 W144056/000012 at TCP/IP 192.168.99.14)
TRX1 AUX  output -> open
TRX2 NORM output -> input 1 of transmitter 1 (BLA2H 200-900 W149107/000014 at TCP/IP 192.168.99.15)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 4 (AV4 BLA2BB500 15-600 W152248/000019 at TCP/IP 192.168.99.12)
TRX3 AUX  output -> open
TRX4 NORM output -> input 2 of transmitter 4 (AV4 BLA2BB500 15-600 W152248/000019 at TCP/IP 192.168.99.12)
TRX4 AUX  output -> open
TRX5 NORM output -> input 1 of transmitter 3 (AV4 BLABB500 15-600 W144059/000058 at TCP/IP 192.168.99.13)
TRX5 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLA2H 200-900 W149107/000014 at TCP/IP 192.168.99.15:
- amplifier 2H-250W uses blanking 2

transmitter 2 = AV4 BLAH500 700-900 W144056/000012 at TCP/IP 192.168.99.14:
- amplifier 1H-500W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 3 = AV4 BLABB500 15-600 W144059/000058 at TCP/IP 192.168.99.13:
- amplifier B-500W uses blanking 5

transmitter 4 = AV4 BLA2BB500 15-600 W152248/000019 at TCP/IP 192.168.99.12:
- amplifier B-500W uses blanking 3
- amplifier B-500W uses blanking 4

transmitter 5 = BSMS/2 LOCK TRANSCEIVER 800 Z109893/00256 at TCP/IP 192.168.99.11:
- amplifier 2H-5W needs no blanking


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 19F1H -> REC1
Tune-TRX2 -> 2H          -> REC2
Tune-TRX3 -> 13C         -> REC3
Tune-TRX3 -> HPLNA BB31P -> REC3
Tune-TRX4 -> 15N         -> REC4
Tune-TRX4 -> HPLNA BB31P -> REC4
Tune-TRX5 -> 31P         -> REC5

