CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.1/conf/instr/spect/uxnmr.info
Date         : Mon Apr 28 11:27:14 2014
Release      : TopSpin Acquisition Version 3.1-pl7
Installed in : /opt/topspin3.1
Host         : IRAM-CA-004237
OS           : CentOS release 5.8 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : joel (joel)
Description  : Avance-AV 700
Location     : 
System       : Avance-AV NMR spectrometer
1H-frequency : 700.13 MHz
Order Number : 
Configured in: /opt/topspin3.1/conf/instr/spect

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 3 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 4 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU-E Z102520/00288 ECL 02.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 120924

Gcu: GCU3_SlowIF

AQS: connected to spect:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AV  R  4.4 REC-1  AQS RXAD1000 Z102118/172 ECL 04.04
     3   0x34 0xc1   0x1        X  0.4 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x28   0x4    BH  S  6.0 SGU-1  AQS SGU1000 Z003330/01160 ECL 6.0
     5   0x25 0x28   0x4    BH  S  6.0 SGU-2  AQS SGU1000 Z003330/01163 ECL 6.0
     6   0x26 0x28   0x4    BH  S  7.0 SGU-3  AQS SGU1000 Z003330/01223 ECL 7.0
     7   0x27 0x28   0x4    BH  S  7.0 SGU-4  AQS SGU1000 Z003330/01204 ECL 7.0
     8   0x3c  0x4     0        Y  1.0 ROUT-1 Avance Router 3/5
    23   0x20 0xc6     0        B  1.1 AQS/2  AQS/2 chassis
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 Avance-Router

Amplifier Control Board:  connected to spect:/dev/tty20


Amplifiers (ACB configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        X      500    N  (V=ff) BLAXH2H 500/100/250 W1345081/9/20051128
   2      1         2       1H      100    N  (-""-) BLAXH2H 500/100/250 W1345081/9/20051128
   3      2         1        X      500    N  (V=ff) BLAX 500 W1345070/432/20050420
   6      3         1       2H      250    N         BLAXH2H 500/100/250 W1345081/9/20000000



- Type: BSMS/1
- absolute lockshift frequency =  12525782 Hz
- GAB type = GAB
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)

Cryo Controller CRCO: device connected to spect:/dev/tty06

Lock: device connected to spect:/dev/tty03

Eurotherm VTU: device connected to spect:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to spect:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AP
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003463, SN=00101 from 20070713
    Module  2 : XBB19F 2HS
                 PN=Z003507, SN=00116 from 20051020
    Module  3 : 13C
                 PN=Z003525, SN=00050 from 20050525
    Module  4 : 15N
                 PN=Z003531, SN=00011 from 20060106
    Module  5 : 2H
                 PN=Z003474, SN=00088 from 20051031


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



