CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Mon Jul 18 11:12:05 2022
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : CZC5064J8K
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v2 @ 3.70GHz (8 cores at 1480 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III HD 700 NMR spectrometer
1H-frequency : 700.13 MHz
Description  : CABINET 700 HD X OB
Location     : Health Canada, Ottawa
Bruker Order : 10193388
Configured in: CZC5064J8K:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/04589 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.3 REC-1  AQS RXAD/2 1000 Z130589/356 ECL 00.03
     3   0x34 0xda   0x1        X  2.2 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00508 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00509 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0347 W1345097/0347 ECL 20:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0347 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/2527 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010486 ECL 50
BLA_W1345093_0791 W1345093/0791 ECL 12:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0791 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/5016 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010602 ECL 50
LTRX Z109891/00316 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00316 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20170712
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00316 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/02632 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/02956 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty04

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.9%/0.1deg, reflection meter)
                PN=Z103206, SN=00328 from 20150217
    Module  2 : 2H
                PN=Z003474, SN=00424 from 20150107
    Module  3 : XBB19F 2HS
                PN=Z003507, SN=00943 from 20150212
    Module  4 : XBB19F 2HS
                PN=Z003507, SN=00942 from 20150109
    Module  5 : 13C
                PN=Z003525, SN=00321 from 20141219
    Module  6 : 15N
                PN=Z003531, SN=00322 from 20150106



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> open
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0791 at TCP/IP 149.236.99.91)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0347 at TCP/IP 149.236.99.92)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0791 at TCP/IP 149.236.99.91)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0347 at TCP/IP 149.236.99.92)
SGU4 NORM output -> input 3 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0791 at TCP/IP 149.236.99.91)
SGU4 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0347 at TCP/IP 149.236.99.92)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0347 at TCP/IP 149.236.99.92:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 2 = BLAX500 E 6-365MHZ INR W1345093/0791 at TCP/IP 149.236.99.91:
- amplifier X-500W uses blanking 4

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 700 Z109891/00316 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


