CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.5/conf/instr/spect/uxnmr.info
Date         : Mon May 29 14:14:57 2023
Release      : TopSpin 3.6.5
Installed in : /opt/topspin3.6.5
Host         : CZC2057FGX
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) W-2223 CPU @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III HD 800 NMR spectrometer
1H-frequency : 799.86 MHz
Description  : Avance HDX 800
Location     : The Francis Crick Institute
Bruker Order : 10096492
Configured in: CZC2057FGX:/opt/topspin3.6.5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.92
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU Z100977/03333 ECL 07.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.2 REC-1  AQS RXAD/2 1000 Z130589/14 ECL 00.02
     3   0x34 0xda   0x1        X  0.2 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00216 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00209 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345500_0025 W1345500/0025 ECL 20:
- TCP/IP address = 149.236.99.95
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 800-1000MHZ INR: W1345500/0025 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/5554 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011363 ECL 60
BLA_W1345529_0133 W1345529/0133 ECL 01:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0133 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2582 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7795 ECL 50
LTRX Z109893/00047 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00047 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20220429
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00047 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01387 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01597 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.92:/dev/tty04
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.92:/dev/tty01

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 149.236.99.55

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.8%/0.0deg, reflection meter)
                PN=Z103208, SN=00055 from 20130426
    Module  2 : 2H
                PN=Z003476, SN=00169 from 20130404
    Module  3 : XBB31P 2HS
                PN=Z003509, SN=00195 from 20130326
    Module  4 : XBB31P 2HS
                PN=Z003509, SN=00194 from 20130326
    Module  5 : 13C
                PN=Z003527, SN=00131 from 20130318
    Module  6 : 15N
                PN=Z003533, SN=00128 from 20130318



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0025 at TCP/IP 149.236.99.95)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0133 at TCP/IP 149.236.99.94)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0025 at TCP/IP 149.236.99.95)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0133 at TCP/IP 149.236.99.94)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0025 at TCP/IP 149.236.99.95)
SGU4 NORM output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0025 at TCP/IP 149.236.99.95)
SGU4 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H500/100/250 E 800-1000MHZBLAX1000 E 6-405MHZ INR OUTR W1345500/0025 at TCP/IP 149.236.99.95:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0133 at TCP/IP 149.236.99.94:
- amplifier X-1000W uses blanking 3
- amplifier X-300W uses blanking 3

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 800 Z109893/00047 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0133 at TCP/IP 149.236.99.94:
- amplifier X-1000W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


