CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.2/conf/instr/spect/uxnmr.info
Date         : Thu Apr  7 15:14:48 2022
Release      : TopSpin 3.6.2
Installed in : /opt/topspin3.6.2
Host         : nmr900.bioz.unibas.ch
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) W-2123 CPU @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmr (NMR User)
System       : Avance III HD 900 NMR spectrometer
1H-frequency : 900.18 MHz
Description  : AVHD900DX
Location     : Biozentrum, Universitaet Basel, Raum U3.170
Bruker Order : 10087366
Configured in: nmr900.bioz.unibas.ch:/opt/topspin3.6.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 5
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU1: AQS DRU-E Z102520/03791 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.2 REC-1  AQS RXAD/2 1000 Z130589/119 ECL 00.02
     3   0x34 0xda   0x1        X  0.2 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00219 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00210 ECL 01.03 FPGA-Vs=20131031
     6   0x28 0x33     0        S  1.3 SGU-3  AQS SGU/3 1200 (2CH) Z117130/00203 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345529_0144 W1345529/0144 ECL 01:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0144 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2625 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/8014 ECL 50
BLA_W1345097_0272 W1345097/0272 ECL 20:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0272 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1846 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7406 ECL 50
BLA_W1345093_0705 W1345093/0705 ECL 12:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0705 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2620 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7944 ECL 50
LTRX Z109895/00016 ECL 01.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 900: Z109895/00016 ECL 01.01

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0107
- TCP/IP address   = 149.236.99.91
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210212
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 900: Z109895/00016 ECL 01.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01847 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/02026 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty04

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.90:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.3%/0.2deg, reflection meter)
                PN=Z103209, SN=00021 from 20131204
    Module  2 : 2H
                PN=Z003477, SN=00054 from 20131119
    Module  3 : XBB31P 2HS
                PN=Z003510, SN=00056 from 20131209
    Module  4 : 13C
                PN=Z003528, SN=00039 from 20131119
    Module  5 : 15N
                PN=Z003534, SN=00042 from 20131120



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected via DPP to GREAT 3-10 Gradient Amplifier Unit W1213762/0107

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0272 at TCP/IP 149.236.99.93)
SGU1 AUX  output -> input 2 of transmitter 3 (BLAX500 E 6-365MHZ INR W1345093/0705 at TCP/IP 149.236.99.92)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0272 at TCP/IP 149.236.99.93)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 3 (BLAX500 E 6-365MHZ INR W1345093/0705 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0272 at TCP/IP 149.236.99.93)
SGU4 NORM output -> input 1 of transmitter 1 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0144 at TCP/IP 149.236.99.94)
SGU4 AUX  output -> input 3 of transmitter 3 (BLAX500 E 6-365MHZ INR W1345093/0705 at TCP/IP 149.236.99.92)
SGU5 NORM output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0272 at TCP/IP 149.236.99.93)
SGU5 AUX  output -> input 2 of transmitter 1 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0144 at TCP/IP 149.236.99.94)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0144 at TCP/IP 149.236.99.94:
- amplifier X-1000W uses blanking 4
- amplifier X-300W uses blanking 4

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ BLAX500 E 6-365MHZ INR W1345097/0272 at TCP/IP 149.236.99.93:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 3 = BLAX500 E 6-365MHZ INR W1345093/0705 at TCP/IP 149.236.99.92:
- amplifier X-500W uses blanking 3

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 900 Z109895/00016 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 1 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0144 at TCP/IP 149.236.99.94:
- amplifier X-1000W at blanking 4 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


