CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2_pl6/conf/instr/Bruker_default_avIII600/uxnmr.info
Date         : Mon Jun  2 10:56:48 2014
Release      : TOPSPIN Version 3.2-pl6
Installed in : /opt/topspin3.2_pl6
Host         : prot-600b
OS           : CentOS release 5.8 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : nmrsu (NMR Administrator (nmrsu))
Description  : Avance III 600
Location     : 
System       : Avance III NMR spectrometer
1H-frequency : 600.25 MHz
Order Number : 
Configured in: /opt/topspin3.2_pl6/conf/instr/Bruker_default_avIII600

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.251
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/00870 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130125 (needs update to version 131205)
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x3    AW  R  3.0 REC-1  AQS RXAD600 Z102117/418 ECL 03.00
     3   0x34 0xc0   0x1        X  2.0 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AD  S  2.1 SGU-1  AQS SGU/2 600 Z103081/00611 ECL 02.01 FPGA-Vs=AE
     5   0x25 0x19   0x8    AD  S  2.1 SGU-2  AQS SGU/2 600 Z103081/00613 ECL 02.01 FPGA-Vs=AE
     6   0x26 0x19   0x8    AD  S  2.1 SGU-3  AQS SGU/2 600 Z103081/00825 ECL 02.01 FPGA-Vs=AE
     7   0x27 0x19   0x8    AD  S  2.1 SGU-4  AQS SGU/2 600 Z103081/00817 ECL 02.01 FPGA-Vs=AE
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  2.1 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0164 W1345096/0164 ECL 1:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ: W1345096/0164 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0254 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/0164 ECL 2
BLA_W1345092_0151 W1345092/0151 ECL 0:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ: W1345092/0151 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0512 ECL 0
- Controller     = BLA CONTROL BOARD 6 1V V-USB: W1522041/0337 ECL 2

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130627
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS2-SB
- 2HTX Amplifier: not available
- Lock: installed

Eurotherm VTU: device connected to 149.236.99.251:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AO
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003462, SN=00543 from 20070719
    Module  2 : XBB19F 2HS
                 PN=Z003506, SN=00601 from 20070709
    Module  3 : 2H
                 PN=Z003473, SN=00543 from 20070716
    Module  4 : 13C
                 PN=Z003524, SN=00401 from 20071221
    Module  5 : 15N
                 PN=Z003530, SN=00294 from 20071207


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ W1345092/0151 at TCP/IP 149.236.99.249)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAX300 E 6-365MHZ W1345092/0151 at TCP/IP 149.236.99.249)
SGU4 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ W1345092/0151 at TCP/IP 149.236.99.249)
SGU4 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250) amplifier X-300W uses blanking 1
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0164 at TCP/IP 149.236.99.250) amplifier 2H-150W needs no blanking
transmitter 2 (BLAX300 E 6-365MHZ W1345092/0151 at TCP/IP 149.236.99.249) amplifier X-300W uses blanking 3

