CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.2/conf/instr/spect/uxnmr.info
Date         : Fri Apr 29 12:22:36 2022
Release      : TopSpin 3.6.2
Installed in : /opt/topspin3.6.2
Host         : nmr600m.bioz.unibas.ch
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Core(TM) i7-6700 CPU @ 3.40GHz (8 cores at 900 MHz with Hyperthreading)
User         : ledann00 (Anna Leder)
System       : Avance III HD 600 NMR spectrometer
1H-frequency : 600.13 MHz
Description  : AV600HD
Location     : Biozentrum Basel, 181A, 1. Stock
Bruker Order : 10131070
Configured in: nmr600m.bioz.unibas.ch:/opt/topspin3.6.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 5
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU1: AQS DRU-E Z102520/03685 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.2 REC-1  AQS RXAD/2 600 Z130588/702 ECL 00.02
     3   0x34 0xd6   0x1        X  3.0 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/01195 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x32     0        S  2.2 SGU-2  AQS SGU/3 600 (2CH) Z117129/01197 ECL 02.02 FPGA-Vs=20131031
     6   0x28 0x32     0        S  2.2 SGU-3  AQS SGU/3 600 (2CH) Z117129/01178 ECL 02.02 FPGA-Vs=20131031
     9   0x36 0xc8     0        A  0.1 BLA-1  AQS 2H-TX BD 500-1000 Z103551/00035 ECL 00.01
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0687 W1345093/0687 ECL 12:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0687 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2560 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7778 ECL 50
BLA_W1345527_0006 W1345527/0006 ECL 12:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAH500 E 500-600MHZ INR OUTR: W1345527/0006 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2562 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7759 ECL 50
BLA_W1345094_0129 W1345094/0129 ECL 11:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLA2X500 E 6-365MHZ INR: W1345094/0129 ECL 11
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/2021 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7750 ECL 50
LTRX Z109890/00443 ECL 03.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00443 ECL 03.01

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0157
- TCP/IP address   = 149.236.99.91
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210212
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00443 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01710 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01725 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty05

MAS2 control unit: connected to 149.236.99.90:/dev/tty04
MAS2: device not yet configured
MAS1: device could not be configured

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.6%/0.1deg, reflection meter)
                PN=Z103205, SN=00251 from 20130821
    Module  2 : 2H
                PN=Z003473, SN=01043 from 20130816
    Module  3 : XBB19F 2HS
                PN=Z003506, SN=01288 from 20131029
    Module  4 : XBB19F 2HS
                PN=Z003506, SN=01275 from 20130923
    Module  5 : 13C
                PN=Z003524, SN=01154 from 20170207
    Module  6 : 15N
                PN=Z003530, SN=00971 from 20151014



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected via DPP to GREAT 3-10 Gradient Amplifier Unit W1213762/0157

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 3 (BLA2X500 E 6-365MHZ INR W1345094/0129 at TCP/IP 149.236.99.92)
SGU1 AUX  output -> input 1 of transmitter 5 (AQS 2H-TX BD 500-1000 Z103551/35)
SGU2 NORM output -> input 1 of transmitter 2 (BLAH500 E 500-600MHZ INR OUTR W1345527/0006 at TCP/IP 149.236.99.93)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 2 of transmitter 3 (BLA2X500 E 6-365MHZ INR W1345094/0129 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 2 of transmitter 2 (BLAH500 E 500-600MHZ INR OUTR W1345527/0006 at TCP/IP 149.236.99.93)
SGU4 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0687 at TCP/IP 149.236.99.94)
SGU4 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0687 at TCP/IP 149.236.99.94)
SGU5 NORM output -> input 3 of transmitter 3 (BLA2X500 E 6-365MHZ INR W1345094/0129 at TCP/IP 149.236.99.92)
SGU5 AUX  output -> input 3 of transmitter 2 (BLAH500 E 500-600MHZ INR OUTR W1345527/0006 at TCP/IP 149.236.99.93)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0687 at TCP/IP 149.236.99.94:
- amplifier X-500W uses blanking 4

transmitter 2 = BLAH500 E 500-600MHZ INR OUTR W1345527/0006 at TCP/IP 149.236.99.93:
- amplifier 1H-500W uses blanking 2
- amplifier 1H-50W uses blanking 2

transmitter 3 = BLA2X500 E 6-365MHZ INR W1345094/0129 at TCP/IP 149.236.99.92:
- amplifier X-500W uses blanking 1
- amplifier X-500W uses blanking 3

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/00443 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking

transmitter 5 = AQS 2H-TX BD 500-1000 Z103551/35:
- amplifier 2H-100W uses blanking 8


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 2 = BLAH500 E 500-600MHZ INR OUTR W1345527/0006 at TCP/IP 149.236.99.93:
- amplifier 1H-500W at blanking 2 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


