CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Thu Nov  2 10:13:31 2023
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : NMR700
OS           : CentOS release 5.10 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2527 MHz)
User         : Donaldson (Logan Donaldson)
System       : Avance III 700 NMR spectrometer
1H-frequency : 700.28 MHz
Description  : Avance III 700
Bruker Order : 10293360
Configured in: NMR700:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.253
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU1: AQS DRU-E Z102520/02237 ECL 06.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AW  R  5.0 REC-1  AQS RXAD1000 Z102118/281 ECL 05.00
     3   0x34 0xc9   0x1        X  1.2 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x29   0x8    AE  S  3.6 SGU-1  AQS SGU/2 1000 Z103082/01061 ECL 03.06 FPGA-Vs=AF
     5   0x25 0x29   0x8    AE  S  3.5 SGU-2  AQS SGU/2 1000 Z103082/00778 ECL 03.05 FPGA-Vs=AF
     6   0x26 0x29   0x8    AE  S  3.5 SGU-3  AQS SGU/2 1000 Z103082/00779 ECL 03.05 FPGA-Vs=AF
     7   0x27 0x29   0x8    AE  S  3.5 SGU-4  AQS SGU/2 1000 Z103082/00780 ECL 03.05 FPGA-Vs=AF
    21   0x21 0xcf     0        P 10.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0391 W1345093/0391 ECL 1:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0391 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1441 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5463 ECL 50
BLA_W1345097_0170 W1345097/0170 ECL 10:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0170 ECL 10
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/001096 ECL 00
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/005470 ECL 60
LTRX Z109891/00027 ECL 01.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00027 ECL 01.00

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0179
- TCP/IP address   = 149.236.99.248
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20190521
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00027 ECL 01.00
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03609 ECL 05.02
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00304 ECL 01.01

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Prodigy Control Unit: PCU - LNP PRODIGY UNIT Z127349/631
- TCP/IP address   = 149.236.99.247

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 1H (virtual 50 Ohm reference: 100.0%/-0.2deg, reflection meter)
                PN=Z103206, SN=00039 from 20101103
    Module  2 : 2H
                PN=Z003474, SN=00639 from 20110106
    Module  3 : XBB19F 2HS
                PN=Z003507, SN=00613 from 20110111
    Module  4 : 13C
                PN=Z003525, SN=00116 from 20100621
    Module  5 : 15N
                PN=Z003531, SN=00108 from 20100615



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected via DPP to GREAT 3-10 Gradient Amplifier Unit W1213762/0179

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0170 at TCP/IP 149.236.99.249)
SGU1 AUX  output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0391 at TCP/IP 149.236.99.250)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0170 at TCP/IP 149.236.99.249)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0170 at TCP/IP 149.236.99.249)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0391 at TCP/IP 149.236.99.250)
SGU4 NORM output -> input 3 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0391 at TCP/IP 149.236.99.250)
SGU4 AUX  output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0170 at TCP/IP 149.236.99.249)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0391 at TCP/IP 149.236.99.250:
- amplifier X-500W uses blanking 3

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0170 at TCP/IP 149.236.99.249:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 700 Z109891/00027 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


