CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Mon Jan 17 10:03:12 2022
Release      : TopSpin 4.1.0
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.1.146.20201002
CPU          : Intel(R) Core(TM) i7-4700EQ CPU @ 2.40GHz (8 cores at 1970 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 850 NMR spectrometer
1H-frequency : 850.25 MHz
Description  : Avance Neo 850
Bruker Order : 415443
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- EPU/2: AV4 EPU/2 Embedded Processing Unit H153448F1/01120 ECL 01.04
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/03756 ECL 02.01
  Location: slot 1 in rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20190906112554
  Devices: MTD at /dev/mtd2, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/03758 ECL 02.01
  Location: slot 2 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20190906112554
  Devices: MTD at /dev/mtd11, DRX at /dev/bbu/drx4.5, RTD at /dev/bbu/rtd4.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/03759 ECL 02.01
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.22 via PCIe #5
  Firmware Version: 20190906112554
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx5.5, RTD at /dev/bbu/rtd5.4
  Sequencer: FCube
  - FCube3
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/03760 ECL 02.01
  Location: slot 4 in rack 1
  Connection: at IP 192.168.180.26 via PCIe #6
  Firmware Version: 20190906112554
  Devices: MTD at /dev/mtd29, DRX at /dev/bbu/drx6.5, RTD at /dev/bbu/rtd6.4
  Sequencer: FCube
  - FCube4
- GTU: AV4 GT-CONTROLLER UNIT Z148393/01187 ECL 01.02
  Location: slot 6 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20190906085855
  Devices: MTD at /dev/mtd37, RTD at /dev/bbu/rtd9.4, GPROC at /dev/bbu/gproc9.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- PSM-A: AV4 PSM-A Z149510/01539 ECL 02.01
- HPPR/2 COVER2: HPPR/2 Cover2 Z124567/03313 ECL 00.05
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.7%/0.2deg, reflection meter without CRP-Bias capability)
                  PN=Z105203, SN=00402 from 20180814
      Module  2 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111097, SN=00212 from 20190315
      Module  3 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111097, SN=00209 from 20190214
      Module  4 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111097, SN=00210 from 20190214
  
- HPLNA 19F1H: HPLNA 1H MODULE 850 Z105203/00402 ECL 06.02
- HPLNA BB31P: HPLNA XBB 31P MODULE 850 Z111097/00212 ECL 04.04
- HPLNA BB31P: HPLNA XBB 31P MODULE 850 Z111097/00209 ECL 04.04
- HPLNA BB31P: HPLNA XBB 31P MODULE 850 Z111097/00210 ECL 04.04
- RACK: AV4 AQS CHASSIS Z149500/01296 ECL 02.00
- PSM-48V: AV4 PSM-48V Z149850/02684 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/01523 ECL 01.01
- FANTRAY: AV4 AQS FAN TRAY Z149501/01236 ECL 00.02
- REF 1200: AV4 REFERENCE 1200 Z148270/01297 ECL 02.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144059-000372 W144059/000372 ECL 10:
- TCP/IP address = 192.168.99.16
- Firmware VS    = 20181126
- Amplifier      = AV4 BLABB500 15-600: W144059/000372 ECL 10
- Controller     = BLA CONTROL BOARD 7: W133936/022287 ECL 21
BLA-W144060-000115 W144060/000115 ECL 40:
- TCP/IP address = 192.168.99.14
- Firmware VS    = 20160518
- Amplifier      = AV4 BLABB1000 15-600: W144060/000115 ECL 40
- Controller     = BLA CONTROL BOARD 7: W133936/021758 ECL 21
BLA-W144058-000021 W144058/000021 ECL 01:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20160518
- Amplifier      = AV4 BLAH1000 700-900: W144058/000021 ECL 01
- Controller     = BLA CONTROL BOARD 7: W133936/021687 ECL 21
BLA-W144059-000333 W144059/000333 ECL 10:
- TCP/IP address = 192.168.99.11
- Firmware VS    = 20160518
- Amplifier      = AV4 BLABB500 15-600: W144059/000333 ECL 10
- Controller     = BLA CONTROL BOARD 7: W133936/022014 ECL 21

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10
- ELCB firmware version = 20190521
- ELCB = BSMS/2 ELCB: Z100818/08206 ECL 07.02
- Shim System = BOSS-WB
- SCB channels = 40
- Shim matrix file: 272623fb.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 (X2-Y2)Z3 XYZ3
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- 2HTX Amplifier: not available
- Lock: not available
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00784 ECL 05.02
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC-E: Z140144/00233 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10

- Firmware version = 20200617_1039
MAS Control Unit: MAS_H139288_0237
- TCP/IP address   = 192.168.98.2

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99
Line Distribution Unit 2: PDU2
- TCP/IP address   = 192.168.99.101


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 3 (AV4 BLAH1000 700-900 W144058/000021 at TCP/IP 192.168.99.12)
TRX1 AUX  output -> open
TRX2 NORM output -> input 1 of transmitter 1 (AV4 BLABB500 15-600 W144059/000372 at TCP/IP 192.168.99.16)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 4 (AV4 BLABB500 15-600 W144059/000333 at TCP/IP 192.168.99.11)
TRX3 AUX  output -> open
TRX4 NORM output -> input 1 of transmitter 2 (AV4 BLABB1000 15-600 W144060/000115 at TCP/IP 192.168.99.14)
TRX4 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLABB500 15-600 W144059/000372 at TCP/IP 192.168.99.16:
- amplifier B-500W uses blanking 2

transmitter 2 = AV4 BLABB1000 15-600 W144060/000115 at TCP/IP 192.168.99.14:
- amplifier B-1000W uses blanking 4
- amplifier B-100W uses blanking 4

transmitter 3 = AV4 BLAH1000 700-900 W144058/000021 at TCP/IP 192.168.99.12:
- amplifier 1H-1000W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 4 = AV4 BLABB500 15-600 W144059/000333 at TCP/IP 192.168.99.11:
- amplifier B-500W uses blanking 3


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 19F1H -> REC1
Tune-TRX2 -> HPLNA BB31P -> REC2
Tune-TRX3 -> HPLNA BB31P -> REC3
Tune-TRX4 -> HPLNA BB31P -> REC4

