##TITLE= Audit trail, TopSpin 4.1.0
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= nmrsu
$$ /opt/nmrdata/user/moha/nmr/AB40CN_3p2/200/audita.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-09-16 01:47:09.396 +0000>,<nmrsu>,<l1030-ssnmr850>,<go4>,<TopSpin 4.1.0>,
      <acquisition in progress>)
$$ /opt/nmrdata/user/moha/nmr/20210915_AB40CN_3p2/15/audita.txt
(   2,<2021-09-16 03:41:27.903 +0000>,<nmrsu>,<l1030-ssnmr850>,<go4>,<TopSpin 4.1.0>,
      <created by zg on 'Avance Neo 850' (l1030-ssnmr850) by user 'nmrsu'
       on data set with UUID '0134401e-1690-11ec-a533-0013952c0749'
       started at 2021-09-16 01:47:09.422 +0000, POWCHK enabled, PULCHK disabled,
       terminated by command 'stop' at 2021-09-16 03:41:27.902 +0000
       configuration hash MD5:
       C7 E8 2C FA 65 30 75 D7 E1 7A F3 23 67 C7 5D F7
       double data hash MD5: 1K * 128
       2B CF 92 6C 3A 97 D6 EE 2D C1 86 51 FD 70 B7 BC>)
(   3,<2021-09-16 05:41:25.261 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<sertoint>,<TopSpin 4.1.0>,
      <CAT service failure
       sertoint
       data hash MD5: 1K * 128
       D5 EB 9F 4C 92 15 CB 1D A8 66 F7 1F 86 64 33 4B>)
(   4,<2021-09-16 03:55:41.334 +0000>,<nmrsu>,<l1030-ssnmr850>,<go4>,<TopSpin 4.1.0>,
      <raw data deleted by zg>)
(   5,<2021-09-16 03:55:41.335 +0000>,<nmrsu>,<l1030-ssnmr850>,<go4>,<TopSpin 4.1.0>,
      <acquisition in progress>)
(   6,<2021-09-16 18:06:43.580 +0000>,<nmrsu>,<l1030-ssnmr850>,<go4>,<TopSpin 4.1.0>,
      <created by zg on 'Avance Neo 850' (l1030-ssnmr850) by user 'nmrsu'
       on data set with UUID 'f5d0d7fc-16a1-11ec-b885-0013952c0749'
       started at 2021-09-16 03:55:41.364 +0000, POWCHK enabled, PULCHK disabled,
       completed at 2021-09-16 18:06:43.579 +0000
       configuration hash MD5:
       C7 E8 2C FA 65 30 75 D7 E1 7A F3 23 67 C7 5D F7
       double data hash MD5: 1K * 960
       7C C6 3F 40 D4 2C AE 06 1F 04 C8 EB DE 86 BA 7C>)
(   7,<2021-09-16 20:06:40.841 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<sertoint>,<TopSpin 4.1.0>,
      <CAT service failure
       sertoint
       data hash MD5: 1K * 960
       A7 D9 EC ED 6C 85 E5 09 D4 3E 06 A6 DA D5 BF 9E>)
(   8,<2022-08-23 11:06:53.659 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dirdata>,<TopSpin 4.1.0>,
      <CAT service failure
       wrpa from 1 15 "20210915_AB40CN_3p2" "/opt/nmrdata/user/moha/nmr"
       data hash MD5: 1K * 960
       A7 D9 EC ED 6C 85 E5 09 D4 3E 06 A6 DA D5 BF 9E>)
$$ /opt/nmrdata/user/moha/nmr/20210915_AB40CN_3p2/200/audita.txt
(   9,<2022-08-23 11:07:29.328 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 960 to 512
       data hash MD5: 1K * 512
       6F 3E F2 38 55 04 B9 13 39 51 64 4D C5 82 BF 61>)
$$ /opt/nmrdata/user/moha/nmr/AB40CN_3p2/200/audita.txt
(  10,<2022-08-23 11:20:46.016 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 512 to 960
       data hash MD5: 1K * 960
       A7 D9 EC ED 6C 85 E5 09 D4 3E 06 A6 DA D5 BF 9E>)
(  11,<2022-08-23 11:26:19.533 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dirdata>,<TopSpin 4.1.0>,
      <CAT service failure
       wrpa from 1 201 "AB40CN_3p2" "/opt/nmrdata/user/moha/nmr"
       data hash MD5: 1K * 960
       A7 D9 EC ED 6C 85 E5 09 D4 3E 06 A6 DA D5 BF 9E>)
(  12,<2022-08-23 11:26:32.831 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<proc2d>,<TopSpin 4.1.0>,
      <CAT service failure
       addser F2: ALPHA = 1 GAMMA = 1
       201 "AB40CN_3p2" "/opt/nmrdata/user/moha/nmr"
       data hash MD5: 1K * 960
       39 01 93 68 0C 37 DB 46 C6 B5 F6 BF 9B 3D 89 6A>)
(  13,<2022-08-23 12:18:06.710 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 960 to 512
       data hash MD5: 1K * 512
       08 E1 B7 F3 3E 0E 55 A8 00 9E F8 6F EE B7 C0 9F>)
(  14,<2022-08-23 12:18:26.317 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 512 to 960
       data hash MD5: 1K * 960
       39 01 93 68 0C 37 DB 46 C6 B5 F6 BF 9B 3D 89 6A>)
(  15,<2022-08-23 12:18:49.211 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 960 to 512
       data hash MD5: 1K * 512
       08 E1 B7 F3 3E 0E 55 A8 00 9E F8 6F EE B7 C0 9F>)
(  16,<2022-08-23 12:19:24.738 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 512 to 960
       data hash MD5: 1K * 960
       39 01 93 68 0C 37 DB 46 C6 B5 F6 BF 9B 3D 89 6A>)
(  17,<2022-08-23 12:21:01.134 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 960 to 512
       data hash MD5: 1K * 512
       08 E1 B7 F3 3E 0E 55 A8 00 9E F8 6F EE B7 C0 9F>)
(  18,<2022-08-23 12:21:37.362 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 512 to 960
       data hash MD5: 1K * 960
       39 01 93 68 0C 37 DB 46 C6 B5 F6 BF 9B 3D 89 6A>)
(  19,<2022-08-23 12:40:31.461 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 960 to 512
       data hash MD5: 1K * 512
       08 E1 B7 F3 3E 0E 55 A8 00 9E F8 6F EE B7 C0 9F>)
(  20,<2022-09-08 19:35:03.016 +0200>,<nmrsu>,<l1030-ssnmr850.nmr.mpibpc.mpg.de>,<dataserver>,<TopSpin 4.1.0>,
      <CAT service failure
       changed status parameter F1 TD from 512 to 960
       data hash MD5: 1K * 960
       39 01 93 68 0C 37 DB 46 C6 B5 F6 BF 9B 3D 89 6A>)
##END=

$$ hash MD5
$$ 32 CA 56 10 35 FB 1F B5 FD 2D 66 FE 8B 26 7B 47
