CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl6/conf/instr/spect/uxnmr.info
Date         : Mon Nov  7 10:15:09 2022
Release      : TopSpin 3.5 pl 6
Installed in : /opt/topspin3.5pl6
Host         : CZC636B8SQ
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III HD 800 NMR spectrometer
1H-frequency : 798.43 MHz
Description  : CABINET 800 HD X TB
Bruker Order : 10235945
Configured in: CZC636B8SQ:/opt/topspin3.5pl6/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.91
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/05437 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.4 REC-1  AQS RXAD/2 1000 Z130589/461 ECL 00.04
     3   0x34 0xda   0x1        X  3.1 REF-1  
     4   0x24 0x33     0        S  2.2 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00695 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x33     0        S  2.2 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00697 ECL 02.02 FPGA-Vs=20131031
     9   0x36 0xc8     0        A  0.1 BLA-1  AQS 2H-TX BD 500-1000 Z103551/00043 ECL 00.01
    10   0x3c 0xc5     0        Y  1.0 ROUT-1 AQS Router 1/4
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS Router 1/4


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345528_0013 W1345528/0013 ECL 20:
- TCP/IP address = 149.236.99.95
- Firmware VS    = 20120627
- Amplifier      = BLAH500 E 700-900MHZ INR OUTR: W1345528/0013 ECL 20
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/005371 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011526 ECL 60
BLA_W1345093_1172 W1345093/1172 ECL 12:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/1172 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/005515 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011648 ECL 60
BLA_W1345531_0056 W1345531/0056 ECL 02:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAH1000 E 700-900MHZ INR OUTR: W1345531/0056 ECL 02
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/005473 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011714 ECL 60
BLA_W1345529_0264 W1345529/0264 ECL 01:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0264 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/005453 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011762 ECL 60
LTRX Z109893/00245 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00245 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20180919
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 800: Z109893/00245 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03524 ECL 05.02
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03873 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.91:/dev/tty01

MAS Control Unit: MAS_H139288_0244
- TCP/IP address   = 149.236.99.40

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.8%/-0.1deg, reflection meter)
                PN=Z103208, SN=00261 from 20160817
    Module  2 : HPLNA 19F1H (virtual 50 Ohm reference: 100.8%/-0.0deg, reflection meter)
                PN=Z103208, SN=00263 from 20160817
    Module  3 : 2H
                PN=Z003476, SN=00348 from 20160708
    Module  4 : XBB31P 2HS
                PN=Z003509, SN=00490 from 20160712
    Module  5 : HPLNA BB31P (reflection meter)
                PN=Z111096, SN=00215 from 20160920



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/1172 at TCP/IP 149.236.99.94)
SGU1 AUX  output -> input 3 of transmitter 4 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0264 at TCP/IP 149.236.99.92)
SGU2 NORM output -> open
SGU2 AUX  output -> open
SGU3 NORM output -> input 1 of transmitter 4 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0264 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/1172 at TCP/IP 149.236.99.94)
SGU4 NORM output -> input 2 of transmitter 1 (BLAH500 E 700-900MHZ INR OUTR W1345528/0013 at TCP/IP 149.236.99.95)
SGU4 AUX  output -> input of AQS Router 1/4
AQS Router 1/4 output 1 -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/1172 at TCP/IP 149.236.99.94)
AQS Router 1/4 output 2 -> input 2 of transmitter 4 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0264 at TCP/IP 149.236.99.92)
AQS Router 1/4 output 3 -> input 2 of transmitter 3 (BLAH1000 E 700-900MHZ INR OUTR W1345531/0056 at TCP/IP 149.236.99.93)
AQS Router 1/4 output 4 -> input 1 of transmitter 6 (AQS 2H-TX BD 500-1000 Z103551/43)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAH500 E 700-900MHZ INR OUTR W1345528/0013 at TCP/IP 149.236.99.95:
- amplifier 1H-500W uses blanking 1
- amplifier 1H-50W uses blanking 1

transmitter 2 = BLAX500 E 6-365MHZ INR W1345093/1172 at TCP/IP 149.236.99.94:
- amplifier X-500W uses blanking 4

transmitter 3 = BLAH1000 E 700-900MHZ INR OUTR W1345531/0056 at TCP/IP 149.236.99.93:
- amplifier 1H-1000W uses blanking 3
- amplifier 1H-100W uses blanking 3

transmitter 4 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0264 at TCP/IP 149.236.99.92:
- amplifier X-1000W uses blanking 2
- amplifier X-300W uses blanking 2

transmitter 5 = BSMS/2 LOCK TRANSCEIVER 800 Z109893/00245 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking

transmitter 6 = AQS 2H-TX BD 500-1000 Z103551/43:
- amplifier 2H-100W uses blanking 8


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 1 = BLAH500 E 700-900MHZ INR OUTR W1345528/0013 at TCP/IP 149.236.99.95:
- amplifier 1H-500W at blanking 1 can be routed to switchbox output 1 (unknown) and output 2 (unknown)

transmitter 3 = BLAH1000 E 700-900MHZ INR OUTR W1345531/0056 at TCP/IP 149.236.99.93:
- amplifier 1H-1000W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)

transmitter 4 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0264 at TCP/IP 149.236.99.92:
- amplifier X-1000W at blanking 2 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


