CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.4/conf/instr/spect/uxnmr.info
Date         : Mon Oct 24 13:48:06 2022
Release      : TopSpin 3.6.4
Installed in : /opt/topspin3.6.4
Host         : avance500.structure
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : AMD Ryzen 5 5600G with Radeon Graphics (12 cores at 1400 MHz with Hyperthreading)
User         : nmrsu (nmrsu)
System       : Avance III HD 500 NMR spectrometer
1H-frequency : 499.73 MHz
Description  : 500 AVIII HD
Configured in: avance500.structure:/opt/topspin3.6.4/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/03153 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.1 REC-1  AQS RXAD/2 600 Z130588/308 ECL 00.01
     3   0x34 0xd6   0x1        X  2.0 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.0 SGU-1  AQS SGU/3 600 (2CH) Z117129/00416 ECL 02.00 FPGA-Vs=20131031
     5   0x26 0x32     0        S  2.0 SGU-2  AQS SGU/3 600 (2CH) Z117129/00417 ECL 02.00 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.0 PS-1   
    14   0xa1 0x91     0        V  1.1 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0706 W1345093/0706 ECL 12:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0706 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2647 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7909 ECL 50
BLA_W1345096_0921 W1345096/0921 ECL 30:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0921 ECL 30
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1589 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6753 ECL 50
LTRX Z109889/00420 ECL 02.02:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00420 ECL 02.02

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210212
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00420 ECL 02.02
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00219 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01398 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty05

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 149.236.99.55

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.0%/-0.0deg, reflection meter)
                PN=Z103204, SN=00222 from 20121030
    Module  2 : 2H
                PN=Z003472, SN=01120 from 20121120
    Module  3 : XBB19F 2HS
                PN=Z003505, SN=01239 from 20121203
    Module  4 : 13C
                PN=Z003523, SN=00243 from 20121112
    Module  5 : 15N
                PN=Z003529, SN=00201 from 20121126



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 500 W1345096/0921 at TCP/IP 149.236.99.92)
SGU1 AUX  output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0706 at TCP/IP 149.236.99.93)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 500 W1345096/0921 at TCP/IP 149.236.99.92)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 500 W1345096/0921 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0706 at TCP/IP 149.236.99.93)
SGU4 NORM output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 500 W1345096/0921 at TCP/IP 149.236.99.92)
SGU4 AUX  output -> input 3 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0706 at TCP/IP 149.236.99.93)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0706 at TCP/IP 149.236.99.93:
- amplifier X-500W uses blanking 3

transmitter 2 = BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 500 W1345096/0921 at TCP/IP 149.236.99.92:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W uses blanking 4

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 500 Z109889/00420 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


