CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2.7/conf/instr/spect/uxnmr.info
Date         : Wed Jul  1 09:27:41 2020
Release      : TOPSPIN Version 3.2-pl7
Installed in : /opt/topspin3.2.7
Host         : bio700
OS           : CentOS release 5.11 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : shyao (Shenggen Yao)
Description  : Avance III HD 700
Location     : Bio21 Institute Parkville
System       : Avance III NMR spectrometer
1H-frequency : 700.07 MHz
Order Number : 10078531
Configured in: /opt/topspin3.2.7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/03154 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 131205 (needs update to version 150604)
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.1 REC-1  AQS RXAD/2 1000 Z130589/23 ECL 00.01
     3   0x34 0xda   0x1        X  0.1 REF-1  
     4   0x24 0x33     0        S  1.1 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00043 ECL 01.01 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.1 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00048 ECL 01.01 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.0 PS-1   
    14   0xa1 0x91     0        V  1.1 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0244 W1345097/0244 ECL 20:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0244 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1645 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6903 ECL 50
BLA_W1345092_0594 W1345092/0594 ECL 11:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0594 ECL 11
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/002177 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011559 ECL 60
LTRX Z109891/00077 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00077 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00077 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01234 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01399 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty01
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - SampleJet: at TCP/IP address 149.236.99.55


Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.9%/0.0deg, reflection meter)
                 PN=Z103206, SN=00100 from 20121126
    Module  2 : 2H
                 PN=Z003474, SN=00208 from 20121128
    Module  3 : XBB19F 2HS
                 PN=Z003507, SN=00668 from 20121121
    Module  4 : 13C
                 PN=Z003525, SN=00154 from 20121126
    Module  5 : 15N
                 PN=Z003531, SN=00146 from 20121122


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0594 at TCP/IP 149.236.99.249)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253)
SGU3 AUX  output -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0594 at TCP/IP 149.236.99.249)
SGU4 NORM output -> input 3 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0594 at TCP/IP 149.236.99.249)
SGU4 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253) amplifier X-500W uses blanking 1
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0244 at TCP/IP 149.236.99.253) amplifier 2H-250W uses blanking 4
transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0594 at TCP/IP 149.236.99.249) amplifier X-300W uses blanking 3
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 700 Z109891/00077 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

