CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Thu Jun 22 18:10:59 2023
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : gre026374
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1591 MHz with Hyperthreading)
User         : brutsche (BRUTSCHER Bernhard)
System       : Avance III HD 600 NMR spectrometer
1H-frequency : 599.80 MHz
Description  : AVIIIHD-AGIBRU
Location     : IBS2 Grenoble
Bruker Order : 10092953
Configured in: gre026374:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/03362 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.2 REC-1  AQS RXAD/2 1000 Z130589/61 ECL 00.02
     3   0x34 0xda   0x1        X  0.1 REF-1  
     4   0x24 0x33     0        S  2.2 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00709 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00072 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0569 W1345096/0569 ECL 2:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0569 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0901 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/4774 ECL 50
BLA_W1345529_0090 W1345529/0090 ECL 01:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0090 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2362 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7310 ECL 50
LTRX Z109890/01524 ECL 03.02:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/01524 ECL 03.02

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20160329
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/01524 ECL 03.02
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03017 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01630 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

MAS2 control unit: connected to 149.236.99.90:/dev/tty04
- Boot Software        : 20100908
- Application Software : 20120329
- Insert Time          : 10 s
- Eject Time           : 10 s
- Spin Lock Tolerance  : 5 Hz

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 1H (virtual 50 Ohm reference: 98.3%/0.2deg, reflection meter)
                PN=Z103205, SN=00013 from 20080228
    Module  2 : 2H
                PN=Z003473, SN=00383 from 20050517
    Module  3 : XBB19F 2HS
                PN=Z003506, SN=00403 from 20050419
    Module  4 : XBB19F 2HS
                PN=Z003506, SN=00545 from 20070105
    Module  5 : HPLNA BB31P (reflection meter)
                PN=Z111099, SN=00003 from 20130704
    Module  6 : HPLNA BB31P (reflection meter)
                PN=Z111099, SN=00004 from 20130704



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (probably wrong due to failed detection)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX1000 E 6-405MHZ INR OUTR W1345096/0569 at TCP/IP 149.236.99.92)
SGU1 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX1000 E 6-405MHZ INR OUTR W1345096/0569 at TCP/IP 149.236.99.92)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX1000 E 6-405MHZ INR OUTR W1345096/0569 at TCP/IP 149.236.99.92)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0090 at TCP/IP 149.236.99.91)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX1000 E 6-405MHZ INR OUTR W1345096/0569 at TCP/IP 149.236.99.92)
SGU4 NORM output -> open
SGU4 AUX  output -> open

Blanking cable connections (probably wrong due to failed detection)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ BLAX1000 E 6-405MHZ INR OUTR W1345096/0569 at TCP/IP 149.236.99.92:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking

transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0090 at TCP/IP 149.236.99.91:
- amplifier X-1000W uses blanking 3
- amplifier X-300W uses blanking 3

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/01524 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0090 at TCP/IP 149.236.99.91:
- amplifier X-1000W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


