CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Tue Oct 11 11:49:49 2022
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : gre026372
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1864 MHz with Hyperthreading)
User         : amalki (Anas Malki)
System       : Avance III HD 600 NMR spectrometer
1H-frequency : 600.48 MHz
Description  : AV III 600 HD
Location     : IBS Grenoble
Bruker Order : 10096092
Configured in: gre026372:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.96
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/03466 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.2 REC-1  AQS RXAD/2 600 Z130588/566 ECL 00.02
     3   0x34 0xd6   0x1        X  2.0 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/00858 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x32     0        S  2.2 SGU-2  AQS SGU/3 600 (2CH) Z117129/00875 ECL 02.02 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0635 W1345093/0635 ECL 12:
- TCP/IP address = 149.236.99.95
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0635 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2387 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7383 ECL 50
BLA_W1345096_1002 W1345096/1002 ECL 30:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/1002 ECL 30
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1867 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7401 ECL 50
LTRX Z109890/00405 ECL 03.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00405 ECL 03.01

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0145
- TCP/IP address   = 149.236.99.93
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20160329
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00405 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01427 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01695 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.96:/dev/tty04

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.7%/0.4deg, reflection meter)
                PN=Z103205, SN=00783 from 20160816
    Module  2 : 2H
                PN=Z003473, SN=01014 from 20130424
    Module  3 : XBB19F 2HS
                PN=Z003506, SN=01205 from 20130522
    Module  4 : XBB19F 2HS
                PN=Z003506, SN=01204 from 20130416
    Module  5 : 13C
                PN=Z003524, SN=00764 from 20130402
    Module  6 : 15N
                PN=Z003530, SN=00750 from 20130319



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GREAT 3-10 Gradient Amplifier Unit W1213762/0145

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 600 W1345096/1002 at TCP/IP 149.236.99.94)
SGU1 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0635 at TCP/IP 149.236.99.95)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 600 W1345096/1002 at TCP/IP 149.236.99.94)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0635 at TCP/IP 149.236.99.95)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 600 W1345096/1002 at TCP/IP 149.236.99.94)
SGU4 NORM output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 600 W1345096/1002 at TCP/IP 149.236.99.94)
SGU4 AUX  output -> input 3 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0635 at TCP/IP 149.236.99.95)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0635 at TCP/IP 149.236.99.95:
- amplifier X-500W uses blanking 3

transmitter 2 = BLAXH2H300/100/150 E 200-600MHZ BSMS/2 LOCK TRANSCEIVER 600 W1345096/1002 at TCP/IP 149.236.99.94:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W uses blanking 7

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/00405 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


