CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Mon Oct 10 14:16:08 2022
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : gre026384
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1391 MHz with Hyperthreading)
User         : avallet (Alicia VALLET)
System       : Avance III HD 850 NMR spectrometer
1H-frequency : 850.13 MHz
Description  : AVIIIHD
Location     : IBS2 Grenoble
Bruker Order : 10092923
Configured in: gre026384:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.93
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/03619 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.2 REC-1  AQS RXAD/2 1000 Z130589/104 ECL 00.02
     3   0x34 0xda   0x1        X  0.2 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00196 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00189 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0637 W1345093/0637 ECL 12:
- TCP/IP address = 149.236.99.96
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0637 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2400 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7354 ECL 50
BLA_W1345097_0294 W1345097/0294 ECL 20:
- TCP/IP address = 149.236.99.95
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0294 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1948 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7559 ECL 50
LTRX Z109894/00023 ECL 00.03:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 850: Z109894/00023 ECL 00.03

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20160329
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 850: Z109894/00023 ECL 00.03
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01519 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01887 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.93:/dev/tty01
  Error in communication with sample changer: NL 1: 1000 STOP_CHANGER SampleTransporter: SampleCase must not use external lift control. Please correct in 'cf'.
  Using 60 as default for number of holders
- Capacity: 60 holders (assumed)

Cryo Controller CRCO: device connected to 149.236.99.93:/dev/tty04

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.93:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.0%/0.1deg, reflection meter)
                PN=Z105203, SN=00045 from 20130905
    Module  2 : 2H
                PN=Z104078, SN=00032 from 20130909
    Module  3 : XBB31P 2HS
                PN=Z104077, SN=00036 from 20130807
    Module  4 : XBB31P 2HS
                PN=Z104077, SN=00037 from 20130912
    Module  5 : 13C
                PN=Z107393, SN=00025 from 20130906
    Module  6 : 15N
                PN=Z107394, SN=00025 from 20130917



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 850 W1345097/0294 at TCP/IP 149.236.99.95)
SGU1 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0637 at TCP/IP 149.236.99.96)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 850 W1345097/0294 at TCP/IP 149.236.99.95)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0637 at TCP/IP 149.236.99.96)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 850 W1345097/0294 at TCP/IP 149.236.99.95)
SGU4 NORM output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 850 W1345097/0294 at TCP/IP 149.236.99.95)
SGU4 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0637 at TCP/IP 149.236.99.96:
- amplifier X-500W uses blanking 3

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 850 W1345097/0294 at TCP/IP 149.236.99.95:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 850 Z109894/00023 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


