
New TopShim run:

version = topshim 2.0.0
date = 2021-12-22
time = 16:08:04.553
command = topshim  z6off 1d optsolvent coil=1H tuneboff tuneaoff

1D SHIMMING

Parameters:

maximum order = 5
probe = Z123212_0002
solvent = D2O_salt
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 4.70 ppm
optimisation parameters = ls
linewidth 1H = 0.10 Hz
envelope shape / strictness = 2.00 / 200

Results:

initial B0 stdDev = 3.01 Hz
sample size = 2.35 cm, position = -0.08 cm
final B0 stdDev = 2.98 Hz > improvement = 1.0
envelope width = 0.58 Hz
shim changes: 
Z	+9
Z2	+3
Z3	-63
Z4	+107
Z5	+176

duration = 41 sec
completed successfully
finished Wed Dec 22 16:08:42 2021
