CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Fri Aug 29 18:45:05 2025
Release      : TopSpin 4.0.7
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.0.38.20190507
CPU          : Intel(R) Core(TM) i7-4700EQ CPU @ 2.40GHz (8 cores at 2157 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 700 NMR spectrometer
1H-frequency : 700.05 MHz
Description  : AV4 700
Bruker Order : HCAB-70_00025
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- EPU/2: AV4 EPU/2 Embedded Processing Unit H153448F1/00144 ECL 01.02
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00929 ECL 01.05
  Location: in slot 1 of rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd1, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00931 ECL 01.05
  Location: in slot 2 of rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd4, DRX at /dev/bbu/drx4.5, RTD at /dev/bbu/rtd4.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00932 ECL 01.05
  Location: in slot 3 of rack 1
  Connection: at IP 192.168.180.22 via PCIe #5
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd7, DRX at /dev/bbu/drx5.5, RTD at /dev/bbu/rtd5.4
  Sequencer: FCube
  - FCube3
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00541 ECL 01.05
  Location: in slot 4 of rack 1
  Connection: at IP 192.168.180.26 via PCIe #6
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd10, DRX at /dev/bbu/drx6.5, RTD at /dev/bbu/rtd6.4
  Sequencer: FCube
  - FCube4
- GTU: AV4 GT-CONTROLLER UNIT Z148393/00289 ECL 01.01
  Location: in slot 6 of rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20170901114310
  Devices: MTD at /dev/mtd13, RTD at /dev/bbu/rtd9.4, GPROC at /dev/bbu/gproc9.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00657 ECL 01.05
  Location: in slot 7 of rack 1
  Connection: at IP 192.168.180.42 via PCIe #10
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd16, DRX at /dev/bbu/drx10.5, RTD at /dev/bbu/rtd10.4
  Sequencer: FCube
  - FCube5
- PSM-A: AV4 PSM-A Z149510/00318 ECL 01.03
- RACK: AV4 AQS CHASSIS Z149500/00332 ECL 00.03
- PSM-48V: AV4 PSM-48V Z149850/00620 ECL 01.01
- PSM-D: AV4 PSM-D Z149520/00312 ECL 00.02
- FANTRAY: AV4 AQS FAN TRAY Z149501/02059 ECL 00.02
- REF 1200: AV4 REFERENCE 1200 Z148270/00352 ECL 02.01
- HPPR/2 COVER2: HPPR/2 Cover2 Z124567/02483 ECL 00.03
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.7%/0.2deg, reflection meter without CRP-Bias capability)
                  PN=Z103206, SN=00401 from 20171113
      Module  2 : 2H
                  PN=Z003474, SN=00485 from 20171107
      Module  3 : 13C/79Br
                  PN=Z003525, SN=00376 from 20171017
      Module  4 : 15N
                  PN=Z003531, SN=00088 from 20140108
      Module  5 : 31P
                  PN=Z102450, SN=00216 from 20170802
  
- HPLNA 19F1H: HPLNA 1H MODULE 700 Z103206/00401 ECL 02.04
- 2H: HPPR/2 2H MODULE 700 Z003474/00485 ECL 07.00
- 13C/79Br: HPPR/2 13C MODULE 700 Z003525/00376 ECL 08.00
- 15N: HPPR/2 15N MODULE 700 Z003531/00088 ECL 02.02
- 31P: HPPR/2 31P MODULE 700 Z102450/00216 ECL 07.01


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W152248-000035 W152248/000035 ECL 00:
- TCP/IP address = 192.168.99.13
- Firmware VS    = 20160518
- Amplifier      = AV4 BLA2BB500 15-600: W152248/000035 ECL 00
- Controller     = BLA CONTROL BOARD 7: W133936/020079 ECL 30
BLA-W148223-000044 W148223/000044 ECL 01:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20160518
- Amplifier      = AV4 BLABBH2H 500/100/250 700-900: W148223/000044 ECL 01
- Controller     = BLA CONTROL BOARD 7: W133936/020163 ECL 21
LTRX Z109891/01087 ECL 02.01:
- TCP/IP address = 192.168.99.11
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/01087 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11
- ELCB firmware version = 20180620
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- Shim matrix file: 292722da.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 Z7 Z8 XZ5 YZ5 (X2-Y2)Z3 (X2-Y2)Z4 (X2-Y2)Z5 XYZ3 XYZ4 XYZ5
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/01087 ECL 02.01
- Lock: on L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/04199 ECL 05.02
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/00276 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11

Cryo Cooling Control Unit: RETROFIT-CU - AV4 RETROFIT RS232 CU JAC Z161936/00213
- TCP/IP address   = 192.168.98.2

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99


Gradient Controller cable connections
--------------------------------------------------------------------


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 2 of transmitter 2 (AV4 BLABBH2H 500/100/250 700-900 W148223/000044 at TCP/IP 192.168.99.12)
TRX1 AUX  output -> open
TRX2 NORM output -> input 3 of transmitter 2 (AV4 BLABBH2H 500/100/250 700-900 W148223/000044 at TCP/IP 192.168.99.12)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 2 (AV4 BLABBH2H 500/100/250 700-900 W148223/000044 at TCP/IP 192.168.99.12)
TRX3 AUX  output -> open
TRX4 NORM output -> input 1 of transmitter 1 (AV4 BLA2BB500 15-600 W152248/000035 at TCP/IP 192.168.99.13)
TRX4 AUX  output -> open
TRX5 NORM output -> input 2 of transmitter 1 (AV4 BLA2BB500 15-600 W152248/000035 at TCP/IP 192.168.99.13)
TRX5 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLA2BB500 15-600 W152248/000035 at TCP/IP 192.168.99.13:
- amplifier B-500W uses blanking 4
- amplifier B-500W uses blanking 5

transmitter 2 = AV4 BLABBH2H 500/100/250 700-900 W148223/000044 at TCP/IP 192.168.99.12:
- amplifier B-500W uses blanking 3
- amplifier 1H-100W uses blanking 1
- amplifier 2H-250W uses blanking 2

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 700 Z109891/01087 at TCP/IP 192.168.99.11:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 1 = AV4 BLA2BB500 15-600 W152248/000035 at TCP/IP 192.168.99.13:
- amplifier B-500W at blanking 4 can be routed to switchbox output 1 (unknown) and output 2 (unknown)
- amplifier B-500W at blanking 5 can be routed to switchbox output 3 (unknown) and output 4 (unknown)

transmitter 2 = AV4 BLABBH2H 500/100/250 700-900 W148223/000044 at TCP/IP 192.168.99.12:
- amplifier 1H-100W at blanking 1 can be routed to switchbox output 3 (unknown)
- amplifier 2H-250W at blanking 2 can be routed to switchbox output 4 (unknown)
- amplifier B-500W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 19F1H -> REC1
Tune-TRX2 -> 2H          -> REC2
Tune-TRX3 -> 13C/79Br    -> REC3
Tune-TRX4 -> 15N         -> REC4
Tune-TRX5 -> 31P         -> REC5

