CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Fri Sep  6 13:22:52 2024
Release      : TopSpin 4.4.0
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.4.180.20240301
CPU          : Intel(R) Core(TM) i5-8400H CPU @ 2.50GHz (8 cores at 3612 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 950 NMR spectrometer
1H-frequency : 950.23 MHz
Description  : Avance
Bruker Order : HCAB-96_00002
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- SCU: AV4I SCU SYSTEM CONTROL UNIT Z162978/00466 ECL 02.00
- {EPU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/00466 ECL 02.00
- {GTU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/00466 ECL 02.00
  Location: slot 7 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20210312125813
  - Gradient resolution: 1.0 us
  Devices: MTD at /dev/mtd11, RTD at /dev/bbu/rtd4.4, GPROC at /dev/bbu/gproc4.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06146 ECL 02.03
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx9.5, RTD at /dev/bbu/rtd9.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06147 ECL 02.03
  Location: slot 4 in rack 1
  Connection: at IP 192.168.180.46 via PCIe #11
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd29, DRX at /dev/bbu/drx11.5, RTD at /dev/bbu/rtd11.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06148 ECL 02.03
  Location: slot 5 in rack 1
  Connection: at IP 192.168.180.54 via PCIe #13
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd38, DRX at /dev/bbu/drx13.5, RTD at /dev/bbu/rtd13.4
  Sequencer: FCube
  - FCube3
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06149 ECL 02.03
  Location: slot 6 in rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd2, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube4
- PSM-A: AV4 PSM-A Z149510/02522 ECL 03.01
- HPPR/2 COVER2: HPPR/2 Cover2N Z178831/00081 ECL 00.00
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 1H19F (virtual 50 Ohm reference: 100.1%/-0.4deg, reflection meter with CRP-Bias capability)
                  PN=Z106278, SN=00210 from 20201113
      Module  2 : 2H
                  PN=Z106273, SN=00210 from 20200928
      Module  3 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111099, SN=00210 from 20190417
      Module  4 : 13C/79Br
                  PN=Z106275, SN=00210 from 20200928
      Module  5 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111099, SN=00209 from 20190214
      Module  6 : 15N
                  PN=Z106276, SN=00206 from 20180514
  
- HPLNA 1H19F: HPLNA 1H MODULE 950 Z106278/00210 ECL 06.05
- 2H: HPPR/2 2H MODULE 950 Z106273/00210 ECL 07.00
- HPLNA BB31P: HPLNA XBB 31P MODULE 950 Z111099/00210 ECL 04.04
- 13C/79Br: HPPR/2 13C MODULE 950 Z106275/00210 ECL 08.00
- HPLNA BB31P: HPLNA XBB 31P MODULE 950 Z111099/00209 ECL 04.04
- 15N: HPPR/2 15N MODULE 950 Z106276/00206 ECL 02.02
- RACK: AV4I AQS CHASSIS Z175600/00311 ECL 00.00
- FANTRAY: AV4I AQS FAN TRAY Z175900/00218 ECL 00.00
- PSM-48V: AV4 PSM-48V Z149850/04218 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/02410 ECL 01.01
- REF 1200: AV4 REFERENCE 1200 Z148270/02310 ECL 02.04


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144060-000224 W144060/000224 ECL 41:
- TCP/IP address = 192.168.99.14
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB1000 15-600: W144060/000224 ECL 41
- Controller     = BLA CONTROL BOARD 7: W133936/023526 ECL 40
BLA-W144059-000526 W144059/000526 ECL 11:
- TCP/IP address = 192.168.99.13
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB500 15-600: W144059/000526 ECL 11
- Controller     = BLA CONTROL BOARD 7: W133936/023547 ECL 40
BLA-W162904-000022 W162904/000022 ECL 01:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20210223
- Amplifier      = BLA2H 950-1200: W162904/000022 ECL 01
- Controller     = BLA CONTROL BOARD 7: W133936/023383 ECL 40
BLA-W144271-000015 W144271/000015 ECL 04:
- TCP/IP address = 192.168.99.11
- Firmware VS    = 20210223
- Amplifier      = AV4 BLAH1000 950-1000: W144271/000015 ECL 04
- Controller     = BLA CONTROL BOARD 7: W133936/023497 ECL 40
LTRX Z109896/00209 ECL 01.02:
- TCP/IP address = 192.168.99.10
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 950: Z109896/00209 ECL 01.02

BSMS: BSMS/2 functionality available
- TCP/IP address = 192.168.99.10
- ELCB firmware version = 20231219
- ELCB = BSMS/2 ELCB: Z100818/08984 ECL 07.03
- Backplane = AV4 BSMS CHASSIS: Z152144/01689 ECL 03.01
- Fan tray = AV4 BSMS FAN TRAY: Z152145/01692 ECL 00.02
- Power Supply = AV4 BSMS PSM-B POWER SUPPLY: Z150090/01689 ECL 01.01
- Power Supply 48V 1 = AV4 PSM-48V: Z149850/04219 ECL 01.02
- Variable Power Supply 1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/01969 ECL 01.02
- Power Control = AV4 BSMS POWER CONTROL BOARD: Z150089/01784 ECL 01.00
- SLCB functionality: Available
- GAB Z-Gradient = AV4 GAB/2 GRADIENT AMPL BD: Z155150/01953 ECL 00.01
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- Shim System = BOSS3-SB
- SCB channels = 40
- SCB1 = BSMS/2 SCB20: Z102930/14028 ECL 05.00
- SCB2 = BSMS/2 SCB20: Z102930/14051 ECL 05.00
- Shim matrix file: 292722de.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 Z7 Z8 XZ5 YZ5 (X2-Y2)Z3 (X2-Y2)Z4 (X2-Y2)Z5 XYZ3 XYZ4 XYZ5
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 950: Z109896/00209 ECL 01.02
- Lock: On L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/06099 ECL 05.05
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/01969 ECL 01.02
- SampleMail = SM SAMPLEMAIL PLUS 1030 KPL.: Z123384/285 ECL 0.09

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10
-  = SM SAMPLEMAIL PLUS 1030 KPL.: Z123384/285 ECL 0.09
- VTC active channel 1 = BSMS/2 VTA CRP: Z116923/01487 ECL 02.02
- VTC active channel 2 = BSMS/2 VTA SACA: Z141200/00268 ECL 00.05
- VTC accessory channel 1 = BCU II: Z117485/0675 ECL 01.01
- VTC accessory channel 2 = N2-LEVELSONDE 7/2142/1560 BSNL (900): Z126074/00000 ECL 00.00

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10

Cryo Cooling Control Unit: CU5 - COOLING UNIT/5 Z159073/092
- TCP/IP address   = 192.168.98.6
- BSNL available   = no

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99
Line Distribution Unit 2: PDU2
- TCP/IP address   = 192.168.99.101

Magnet System:
- Magnet  : BR086095271
- Cryostat: M1009520
- Polarity: SN (Bruker)


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 4 (AV4 BLAH1000 950-1000 W144271/000015 at TCP/IP 192.168.99.11)
TRX1 AUX  output -> open
TRX2 NORM output -> input 1 of transmitter 3 (BLA2H 950-1200 W162904/000022 at TCP/IP 192.168.99.12)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 2 (AV4 BLABB500 15-600 W144059/000526 at TCP/IP 192.168.99.13)
TRX3 AUX  output -> open
TRX4 NORM output -> input 1 of transmitter 1 (AV4 BLABB1000 15-600 W144060/000224 at TCP/IP 192.168.99.14)
TRX4 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLABB1000 15-600 W144060/000224 at TCP/IP 192.168.99.14:
- amplifier B-1000W uses blanking 4
- amplifier B-100W uses blanking 4

transmitter 2 = AV4 BLABB500 15-600 W144059/000526 at TCP/IP 192.168.99.13:
- amplifier B-500W uses blanking 3

transmitter 3 = BLA2H 950-1200 W162904/000022 at TCP/IP 192.168.99.12:
- amplifier 2H-250W uses blanking 2

transmitter 4 = AV4 BLAH1000 950-1000 W144271/000015 at TCP/IP 192.168.99.11:
- amplifier 1H-1000W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 5 = BSMS/2 LOCK TRANSCEIVER 950 Z109896/00209 at TCP/IP 192.168.99.10:
- amplifier 2H-5W needs no blanking


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 1H19F -> REC1
Tune-TRX2 -> 2H          -> REC2
Tune-TRX3 -> HPLNA BB31P -> REC3
Tune-TRX3 -> 13C/79Br    -> REC3
Tune-TRX4 -> HPLNA BB31P -> REC4
Tune-TRX4 -> 15N         -> REC4