CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Wed May 15 15:11:09 2024
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : gre026373
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1291 MHz with Hyperthreading)
User         : avallet (VALLET Alicia)
System       : Avance III HD 700 NMR spectrometer
1H-frequency : 700.25 MHz
Description  : Avance III 700
Location     : IBS2 Grenoble
Bruker Order : 10092944
Configured in: gre026373:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.95
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/03376 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.2 REC-1  AQS RXAD/2 1000 Z130589/69 ECL 00.02
     3   0x34 0xda   0x1        X  0.1 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00111 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00120 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0032 W1345097/0032 ECL 00:
- TCP/IP address = 149.236.99.98
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ: W1345097/0032 ECL 00
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/000201 ECL 00
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/000055 ECL 60
BLA_W1345531_0023 W1345531/0023 ECL 02:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAH1000 E 700-900MHZ INR OUTR: W1345531/0023 ECL 02
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2288 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7166 ECL 50
BLA_W1345529_0074 W1345529/0074 ECL 01:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0074 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2285 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7103 ECL 50
LTRX Z109891/00091 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00091 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20220902
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00091 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01437 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01698 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.95:/dev/tty01
- Capacity: 1 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.95:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.7%/-0.1deg, reflection meter)
                PN=Z103206, SN=00119 from 20130625
    Module  2 : 2H
                PN=Z003474, SN=00220 from 20130610
    Module  3 : XBB19F 2HS
                PN=Z003507, SN=00689 from 20130615
    Module  4 : 31P
                PN=Z102450, SN=00022 from 20130515
    Module  5 : 13C
                PN=Z003525, SN=00164 from 20130627
    Module  6 : 15N
                PN=Z003531, SN=00159 from 20130701
    Module  7 : HPLNA BB31P (reflection meter)
                PN=Z111094, SN=00011 from 20130508
    Module  8 : HPLNA BB31P (reflection meter)
                PN=Z111094, SN=00012 from 20130508



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0032 at TCP/IP 149.236.99.98)
SGU1 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0032 at TCP/IP 149.236.99.98)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0032 at TCP/IP 149.236.99.98)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 3 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0074 at TCP/IP 149.236.99.93)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0032 at TCP/IP 149.236.99.98)
SGU4 NORM output -> input 1 of transmitter 2 (BLAH1000 E 700-900MHZ INR OUTR W1345531/0023 at TCP/IP 149.236.99.94)
SGU4 AUX  output -> input 2 of transmitter 3 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0074 at TCP/IP 149.236.99.93)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H500/100/250 E 700-900MHZ W1345097/0032 at TCP/IP 149.236.99.98:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking

transmitter 2 = BLAH1000 E 700-900MHZ INR OUTR W1345531/0023 at TCP/IP 149.236.99.94:
- amplifier 1H-1000W uses blanking 4
- amplifier 1H-100W uses blanking 4

transmitter 3 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0074 at TCP/IP 149.236.99.93:
- amplifier X-1000W uses blanking 3
- amplifier X-300W uses blanking 3

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 700 Z109891/00091 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 2 = BLAH1000 E 700-900MHZ INR OUTR W1345531/0023 at TCP/IP 149.236.99.94:
- amplifier 1H-1000W at blanking 4 can be routed to switchbox output 1 (unknown) and output 2 (unknown)

transmitter 3 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0074 at TCP/IP 149.236.99.93:
- amplifier X-1000W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


