EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
T_NAME		Date_
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 50000000
		REL	"Date_=itodate(DATE)"
		INV_REL	"DATE=datetoi(Date_,DATE)"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		Time
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"Time=itotime(DATE)"
		INV_REL	"DATE=timetoi(Time,DATE)"
		FORMAT	"%14.2f h"
		TEXT	" "
END
NAME		INSTRUM
		TEXT	" "
END
NAME		PROBHD
		FORMAT	"%14.14s"
		TEXT	" "
END
NAME		PULPROG
		TEXT	" "
END
NAME		TD
		TEXT	" "
END
NAME		SOLVENT
		TEXT	" "
END
NAME		NS
		TEXT	" "
END
NAME		DS
		TEXT	" "
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e8
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.3f Hz"
		TEXT	" "
END
T_NAME          FIDRES
                TYPE    R32
                CLASS   ACQU
                SUBRANGE 0.0 100000
                REL     "FIDRES=2*SW*SFO1/TD"
                INV_REL "TD = nextpow(2*SW*SFO1/FIDRES)"
		UNIT	"Hz"
		FORMAT	"%14.6f Hz"
		TEXT	" "
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
		TEXT	" "
END
NAME		RG
		TEXT	" "
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3lf usec"
		TEXT	" "
END
NAME		DE
		FORMAT	"%14.2f usec"
		TEXT	" "
END
NAME		TE
		FORMAT	"%14.1f K"
		TEXT	" "
END
T_NAME		CNST4
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST4=CNST[4]"
INV_REL	"CNST[4]=CNST4"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST12
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST12=CNST[12]"
INV_REL	"CNST[12]=CNST12"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST22
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST22=CNST[22]"
INV_REL	"CNST[22]=CNST22"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST23
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST23=CNST[23]"
INV_REL	"CNST[23]=CNST23"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST24
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST24=CNST[24]"
INV_REL	"CNST[24]=CNST24"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST25
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST25=CNST[25]"
INV_REL	"CNST[25]=CNST25"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST26
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST26=CNST[26]"
INV_REL	"CNST[26]=CNST26"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST27
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST27=CNST[27]"
INV_REL	"CNST[27]=CNST27"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST28
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST28=CNST[28]"
INV_REL	"CNST[28]=CNST28"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST29
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST29=CNST[29]"
INV_REL	"CNST[29]=CNST29"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST31
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST31=CNST[31]"
INV_REL	"CNST[31]=CNST31"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST41
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST41=CNST[41]"
INV_REL	"CNST[41]=CNST41"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		D0
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D0=D[0]"
INV_REL	"D[0]=D0"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D1
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D1=D[1]"
INV_REL	"D[1]=D1"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D10
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D10=D[10]"
INV_REL	"D[10]=D10"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D11
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D11=D[11]"
INV_REL	"D[11]=D11"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D14
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D14=D[14]"
INV_REL	"D[14]=D14"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D16
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D16=D[16]"
INV_REL	"D[16]=D16"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D20
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D20=D[20]"
INV_REL	"D[20]=D20"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D21
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D21=D[21]"
INV_REL	"D[21]=D21"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D22
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D22=D[22]"
INV_REL	"D[22]=D22"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D23
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D23=D[23]"
INV_REL	"D[23]=D23"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D24
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D24=D[24]"
INV_REL	"D[24]=D24"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D25
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D25=D[25]"
INV_REL	"D[25]=D25"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D26
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D26=D[26]"
INV_REL	"D[26]=D26"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		IN0
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"IN0=IN[0]"
INV_REL	"IN[0]=IN0"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		IN10
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"IN10=IN[10]"
INV_REL	"IN[10]=IN10"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		L7
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"L7=L[7]"
INV_REL	"L[7]=L7"
FORMAT	"%14.0f"
TEXT	" "
END
T_NAME		L10
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"L10=L[10]"
INV_REL	"L[10]=L10"
FORMAT	"%14.0f"
TEXT	" "
END
T_NAME		P41
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P41=P[41]"
INV_REL	"P[41]=P41"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
NAME		TDav
		TEXT	" "
END
NAME		ZGOPTNS
		TEXT	" "
END
NAME		SFO1
FORMAT	"%14.7f MHz"
TEXT	" "
END
NAME		NUC1
NONEDIT
TEXT	" "
END
NAME		CPDPRG[1]
TEXT	" "
END
T_NAME		P1
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P1=P[1]"
INV_REL	"P[1]=P1"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P12
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P12=P[12]"
INV_REL	"P[12]=P12"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PCPD1
TYPE	R32
CLASS	ACQU
SUBRANGE 0 1e38
REL	"PCPD1=PCPD[1]"
INV_REL	"PCPD[1]=PCPD1"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PLW1
TYPE	R32
CLASS	ACQU
REL	"PLW1=PLW[1]"
INV_REL	"PLW[1]=PLW1"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW1 "
END
T_NAME		PLW12
TYPE	R32
CLASS	ACQU
REL	"PLW12=PLW[12]"
INV_REL	"PLW[12]=PLW12"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW12 "
END
NAME		SFO2
FORMAT	"%14.7f MHz"
TEXT	" "
END
NAME		NUC2
NONEDIT
TEXT	" "
END
T_NAME		CNST2
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST2=CNST[2]"
INV_REL	"CNST[2]=CNST2"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST3
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST3=CNST[3]"
INV_REL	"CNST[3]=CNST3"
FORMAT	"%14.7f"
TEXT	" "
END
NAME		CPDPRG[2]
TEXT	" "
END
NAME		CPDPRG[5]
TEXT	" "
END
NAME		CPDPRG[6]
TEXT	" "
END
NAME		CPDPRG[7]
TEXT	" "
END
T_NAME		P2
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P2=P[2]"
INV_REL	"P[2]=P2"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P22
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P22=P[22]"
INV_REL	"P[22]=P22"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P23
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P23=P[23]"
INV_REL	"P[23]=P23"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P24
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P24=P[24]"
INV_REL	"P[24]=P24"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P25
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P25=P[25]"
INV_REL	"P[25]=P25"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P26
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P26=P[26]"
INV_REL	"P[26]=P26"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P27
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P27=P[27]"
INV_REL	"P[27]=P27"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PLW2
TYPE	R32
CLASS	ACQU
REL	"PLW2=PLW[2]"
INV_REL	"PLW[2]=PLW2"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW2 "
END
T_NAME		PLW21
TYPE	R32
CLASS	ACQU
REL	"PLW21=PLW[21]"
INV_REL	"PLW[21]=PLW21"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW21 "
END
T_NAME		PLW22
TYPE	R32
CLASS	ACQU
REL	"PLW22=PLW[22]"
INV_REL	"PLW[22]=PLW22"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW22 "
END
T_NAME		PLW23
TYPE	R32
CLASS	ACQU
REL	"PLW23=PLW[23]"
INV_REL	"PLW[23]=PLW23"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW23 "
END
T_NAME		PLW24
TYPE	R32
CLASS	ACQU
REL	"PLW24=PLW[24]"
INV_REL	"PLW[24]=PLW24"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW24 "
END
T_NAME		PLW25
TYPE	R32
CLASS	ACQU
REL	"PLW25=PLW[25]"
INV_REL	"PLW[25]=PLW25"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW25 "
END
T_NAME		PLW26
TYPE	R32
CLASS	ACQU
REL	"PLW26=PLW[26]"
INV_REL	"PLW[26]=PLW26"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW26 "
END
T_NAME		PLW27
TYPE	R32
CLASS	ACQU
REL	"PLW27=PLW[27]"
INV_REL	"PLW[27]=PLW27"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW27 "
END
NAME		SPNAM[23]
TEXT	" "
END
T_NAME		SPOAL23
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL23=SPOAL[23]"
INV_REL	"SPOAL[23]=SPOAL23"
FORMAT	"%14.3f"
TEXT	" "
END
T_NAME		SPOFFS23
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS23=SPOFFS[23]"
INV_REL	"SPOFFS[0]=SPOFFS0"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	" "
END
NAME		SPNAM[25]
TEXT	" "
END
T_NAME		SPOAL25
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL25=SPOAL[25]"
INV_REL	"SPOAL[25]=SPOAL25"
FORMAT	"%14.3f"
TEXT	" "
END
T_NAME		SPOFFS25
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS25=SPOFFS[25]"
INV_REL	"SPOFFS[0]=SPOFFS0"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	" "
END
T_NAME		SPW25
TYPE	R32
CLASS	ACQU
REL	"SPW25=SPW[25]"
INV_REL	"SPW[25]=SPW25"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"shaped pulse power SPW25"
END
NAME		SPNAM[26]
TEXT	" "
END
T_NAME		SPOAL26
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL26=SPOAL[26]"
INV_REL	"SPOAL[26]=SPOAL26"
FORMAT	"%14.3f"
TEXT	" "
END
T_NAME		SPOFFS26
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS26=SPOFFS[26]"
INV_REL	"SPOFFS[0]=SPOFFS0"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	" "
END
NAME		SPNAM[27]
TEXT	" "
END
T_NAME		SPOAL27
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL27=SPOAL[27]"
INV_REL	"SPOAL[27]=SPOAL27"
FORMAT	"%14.3f"
TEXT	" "
END
T_NAME		SPOFFS27
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS27=SPOFFS[27]"
INV_REL	"SPOFFS[0]=SPOFFS0"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	" "
END
NAME		SPNAM[30]
TEXT	" "
END
T_NAME		SPOAL30
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL30=SPOAL[30]"
INV_REL	"SPOAL[30]=SPOAL30"
FORMAT	"%14.3f"
TEXT	" "
END
T_NAME		SPOFFS30
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS30=SPOFFS[30]"
INV_REL	"SPOFFS[0]=SPOFFS0"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	" "
END
T_NAME		SPW30
TYPE	R32
CLASS	ACQU
REL	"SPW30=SPW[30]"
INV_REL	"SPW[30]=SPW30"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"shaped pulse power SPW30"
END
NAME		SFO3
FORMAT	"%14.7f MHz"
TEXT	" "
END
NAME		NUC3
NONEDIT
TEXT	" "
END
NAME		CPDPRG[3]
TEXT	" "
END
T_NAME		P3
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P3=P[3]"
INV_REL	"P[3]=P3"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PCPD3
TYPE	R32
CLASS	ACQU
SUBRANGE 0 1e38
REL	"PCPD3=PCPD[3]"
INV_REL	"PCPD[3]=PCPD3"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PLW3
TYPE	R32
CLASS	ACQU
REL	"PLW3=PLW[3]"
INV_REL	"PLW[3]=PLW3"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW3 "
END
T_NAME		PLW31
TYPE	R32
CLASS	ACQU
REL	"PLW31=PLW[31]"
INV_REL	"PLW[31]=PLW31"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW31 "
END
NAME		SFO4
FORMAT	"%14.7f MHz"
TEXT	" "
END
NAME		NUC4
NONEDIT
TEXT	" "
END
NAME		CPDPRG[4]
TEXT	" "
END
T_NAME		P4
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P4=P[4]"
INV_REL	"P[4]=P4"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PCPD4
TYPE	R32
CLASS	ACQU
SUBRANGE 0 1e38
REL	"PCPD4=PCPD[4]"
INV_REL	"PCPD[4]=PCPD4"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PLW4
TYPE	R32
CLASS	ACQU
REL	"PLW4=PLW[4]"
INV_REL	"PLW[4]=PLW4"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW4 "
END
T_NAME		PLW41
TYPE	R32
CLASS	ACQU
REL	"PLW41=PLW[41]"
INV_REL	"PLW[41]=PLW41"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW41 "
END
NAME		GPNAM[0]
TEXT	" "
END
T_NAME		GPZ0
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ0=GPZ[0]"
INV_REL	"GPZ[0]=GPZ0"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[1]
TEXT	" "
END
T_NAME		GPZ1
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ1=GPZ[1]"
INV_REL	"GPZ[1]=GPZ1"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[2]
TEXT	" "
END
T_NAME		GPZ2
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ2=GPZ[2]"
INV_REL	"GPZ[2]=GPZ2"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[3]
TEXT	" "
END
T_NAME		GPZ3
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ3=GPZ[3]"
INV_REL	"GPZ[3]=GPZ3"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[4]
TEXT	" "
END
T_NAME		GPZ4
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ4=GPZ[4]"
INV_REL	"GPZ[4]=GPZ4"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[5]
TEXT	" "
END
T_NAME		GPZ5
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ5=GPZ[5]"
INV_REL	"GPZ[5]=GPZ5"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[6]
TEXT	" "
END
T_NAME		GPZ6
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ6=GPZ[6]"
INV_REL	"GPZ[6]=GPZ6"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[7]
TEXT	" "
END
T_NAME		GPZ7
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ7=GPZ[7]"
INV_REL	"GPZ[7]=GPZ7"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[8]
TEXT	" "
END
T_NAME		GPZ8
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ8=GPZ[8]"
INV_REL	"GPZ[8]=GPZ8"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[9]
TEXT	" "
END
T_NAME		GPZ9
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ9=GPZ[9]"
INV_REL	"GPZ[9]=GPZ9"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
T_NAME		P50
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P50=P[50]"
INV_REL	"P[50]=P50"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P51
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P51=P[51]"
INV_REL	"P[51]=P51"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P52
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P52=P[52]"
INV_REL	"P[52]=P52"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P53
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P53=P[53]"
INV_REL	"P[53]=P53"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P54
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P54=P[54]"
INV_REL	"P[54]=P54"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P55
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P55=P[55]"
INV_REL	"P[55]=P55"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P56
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P56=P[56]"
INV_REL	"P[56]=P56"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P57
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P57=P[57]"
INV_REL	"P[57]=P57"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P58
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P58=P[58]"
INV_REL	"P[58]=P58"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P59
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P59=P[59]"
INV_REL	"P[59]=P59"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
